# 8232 DECT Eeprom Layout

Table of Contents

## 1. Scope

The purpose of this document is to describe the EEPROM layout and default parameter settings.

## 2. Introduction

All hardware specific parameters must be set up before the unit leaves the factory. As some of the parameters are vital for the operation of the hardware, a set of default parameters must be programmed before the actual hardware fine-tuning can be initiated. This document lists all default parameters with a short description.

## 3. Understanding defaults

Basically two kinds of EEPROM defaults exist: the standard default and the factory default. The factory default presets the EEPROM to an initial state where all adjustment settings are typically lost. The standard default does not alter factory settings like frequency adjustment and charging levels. Furthermore, a number of levels exist. A level is a grouping of the standard and factory default. It's an attribute that can be applied to any EEPROM location. Currently 6 levels exists. If an EEPROM location is a member of factory default, for example level 4, it will only be defaulted if factory and level 4 is specified when a 'default' command is issued. A command in this sense means a call to the default-function in software. This is used to map the Seg parameter of the test-command NVM_INI to a set of EEPROM locations (please note that the level specified in the NVM_INI command is not the same as the level specified in this document). A location may be a member of more than one level, and the levels are also considered when an EEPROM checksum is calculated.

## 4. Layout

This section lists all EEPROM parameters with a short description.

### 4.1. Reading the layout table

#### 4.1.1. Address Column

This column contains the EEPROM address.

- The address is always presented in hexadecimal.
- The notation 'addr1..addr2' indicates an address range starting at addr1 and ending at addr2.

#### 4.1.2. Value Column

This column contains the actual default-value of the location. If the address column indicates an address range, the value column lists the values in address-order.

- Values are always presented in hexadecimal.
- The notation 'xx..xx' indicates that the same value xx is used for all locations.
- The notation '-' indicates that no default-value exists ie. the location is not defaulted.

#### 4.1.3. Type Column

This column specifies the default-type.

- The notation 'f' indicates a factory default-type.
- The notation 's' indicates a standard default-type.
- The notation '1..6' indicates a level 1..6 default-type.
- The notation '-' indicates that the location is not defaulted.

#### 4.1.4. Name Column

This column contains the parameter name.

#### 4.1.5. Description Column

This column contains a short parameter description.

### 4.2. Layout Table

Address | Value | Type | Name | Description
0000..00AA |  |  |  |
Address | Value | Type | Name | Description (Protocol)
0000..0004 | FF FF FF FF FF | f | Ipei | International Personal Equipment Identity.
0005 | 28 | f | BmcModulationDeviation | Modulation volume over the frequency band.
0006..0007 | 60 02 | f | BmcDefaultFrequency | Frequency Adjustment
0008 | 00 | f | RfLMX4x68Length | Defines use of RfLMX4x68Data
0009..000A | 38 00 | fs4 | FixedEmc | The EMC used in the IWU-TO-IWU information elements, see EN 300 175-5, chapter 7.7.23.
000B..001F | - | - | FixedPhoenixInRamSection Reserved | Reserved
0020 | 00 | f | bFreqBandOffset | Offsets the freq band used For EU DECT: 0x00 For DECT 6.0 (US): 0xEE (-18 channels)
0021 | 00 | f | bRssiScanType | DECT 6.0 advanced scan mode 0x00: disable 0x01: enable
0022 | 00 | f | DiversityMode | Antenna diversity mode: 00 : Antenna diversity (if the remote party supports it, i.e. if the remote part sends prolonged preamble) 01: Use antenna 1 always. 02: Use antenna 2 always.
0023 | 28 | f | bRssiLevel_UpperThreshold | DECT 6.0 (US) upper RSSI threshold.
0024 | 20 | f | bRssiLevel_LowerThreshold | DECT 6.0 (US) lower RSSI threshold.
0025 | 61 | fs | PowerParameters | The following bits control the power management: Bit0: LOW_DUTY_CYCLE Bit1: LOW_DUTY_CYCLE_2_MULTIFRAMES Bit2: LOW_DUTY_CYCLE_3_MULTIFRAMES Bit3: LOW_DUTY_CYCLE_4_MULTIFRAMES Bit4: U_PSC Bit5: SCAN_SLEEP Bit6: PAG_ON Bit7: DIV_8
0026 | 3C | fs | CoverageBeepLimit | -
0027 | 01 | fs | ProtocolFeatures3 | RTX internal feature configuration.
0028 | 01 | f | ClSelect | Crystal Phase adjustment Not for adjustment Used internally by the protocol.
0029 | EA | fs | ScFlags |
002A | 00 | f | DectCountry |
002B | 01 | f | dualband_EnableDualBand Search |
002C | 04 | f | handover_NumberOfConsecutive Errors |
002D | 38 | f | handover_NumberOfErrors InMultiframe |
002E | 00 | f | mute_HandoverErrorRssi Offset |
002F | 03 | f | mute_HandoverErrorRssi Offset_Noisy |
0030 | 90 | f | ProtocolFeatures | RTX internal feature configuration.
0031 | 02 | f | ProtocolFeatures2 | RTX internal feature configuration.
0032..0055 | - | - | RfPower4x1 | RF Power settings. Each set of 3 RF registers settings define a power step. Step 0 is maximum power in EU DECT, Step 1 is maximum power in US DECT. The remaining are used for dynamic power control.
0056 | F0 | fs | DelayLocationTime |
0057 | 00 | f | ProtocolFeatures5 | RTX internal feature configuration.
0058..005C | FF FF FF FF FF | fs | ParkA | PARK for registration A
005D..0061 | FF FF FF FF FF | fs | ParkB | PARK for registration B
0062..0066 | FF FF FF FF FF | fs | ParkC | PARK for registration C
0067..006B | FF FF FF FF FF | fs | ParkD | PARK for registration D
006C..0089 | FF..FF | fs | Deprecated_Park |
008A..0093 | FF..FF | fs | Deprecated_ParkExtra |
0094 | FF | fs | PliA | Park Length Indicator for ParkA
0095 | FF | fs | PliB | Park Length Indicator for ParkB
0096 | FF | fs | PliC | Park Length Indicator for ParkC
0097 | FF | fs | PliD | Park Length Indicator for ParkD
0098..009D | FF FF FF FF FF FF | fs | Deprecated_Pli |
009E..009F | FF FF | fs | Deprecated_PliExtra |
00A0..00A3 | - | - | bRfPowerStepsArr |
00A4 | FF | fs | RfFixedPowerLevel |
00A5 | 00 | fs | RfPowerCtrlFlags |
00A6 | 08 | fs | mute_BmcMuteCtrl |
00A7 | C2 | fs | mute_CrcMask |
00A8 | F0 | fs | mute_FullMuteFrameCnt |
00A9 | FF | fs | mute_BmcMuteNumberOfSteps |
00AA | 08 | fs | ProtocolFeatures4 | RTX internal feature configuration.
00AB..31EF |  |  |  |
00AB..00C3 | - | - | EepromInRamReserved | Reserved
00C4 | 00 | fs | InitialTestMode |
00C5 | 07 | f | Bandgap | Calibration of the BandGap reference voltage.
Address | Value | Type | Name | Description (Eeprom Version)
00C6 | 74 | fs | EeVersion | Used to update eeprom when default values are changed. Range: Fixed value
00C7..00C8 | FF FF | fs | DspPatchCodeStartAddr |
00C9 | - | - | BootMode |
00CA..00D9 |  |  | LogError |
00CA..00CB | FF FF | fs | LogError.Error |
00CC..00CD | FF FF | fs | LogError.Line |
00CE..00D1 | FF FF FF FF | fs | LogError.Info |
00D2..00D5 | FF FF FF FF | fs | LogError.Address |
00D6..00D9 | FF FF FF FF | fs | LogError.Timestamp |
00DA..00EE |  |  | LogAssert |
00DA | 00 | fs | LogAssert.NextAssertId |
00DB..00EE | 00..00 | fs | LogAssert.AssertAddress |
00EF | - | - | PxReserved1 | Reserved
00F0 | 28 | f | BmcModulationDeviation Reduced | Reduced RF modulation used with Japan DECT instead of BmcModulationDeviation
00F1..00F3 | - | - | PxReserved1a | Reserved
00F4..011B | - | - | RfLMX4x68Data | Used to patch initialization data for the LMX4168 and LMX4268. Only loaded if RfLMX4x68Length is defined.
011C..0123 | - | - | PxReserved2 | Reserved
0124..0143 |  |  | ProdTest |
0124 | - | - | ProdTest.ProductionData LayoutRevision |
0125 | - | - | ProdTest.BB_Status |
0126 | - | - | ProdTest.RF_Status |
0127 | - | - | ProdTest.SCAN_Status |
0128 | - | - | ProdTest.ProductionYear |
0129 | - | - | ProdTest.ProductionMonth |
012A | - | - | ProdTest.ProductionDay |
012B | - | - | ProdTest.ModelVariant |
012C | - | - | ProdTest.PCB_Version |
012D | - | - | ProdTest.SCH_Version |
012E | - | - | ProdTest.Mechanical_Version |
012F | - | - | ProdTest.Reserved_1 | Reserved
0130 | - | - | ProdTest.RF_Module_Major |
0131 | - | - | ProdTest.RF_Module_Minor |
0132 | - | - | ProdTest.Display_Major |
0133 | - | - | ProdTest.Display_Minor |
0134 | - | - | ProdTest.RAM_Major |
0135 | - | - | ProdTest.RAM_Minor |
0136 | - | - | ProdTest.FLASH_Major |
0137 | - | - | ProdTest.FLASH_Minor |
0138 | - | - | ProdTest.MIC_Major |
0139 | - | - | ProdTest.MIC_Minor |
013A | - | - | ProdTest.EAR_Major |
013B | - | - | ProdTest.EAR_Minor |
013C | - | - | ProdTest.SPEAKER_Major |
013D | - | - | ProdTest.SPEAKER_Minor |
013E..0141 | - | - | ProdTest.PCB_Ser_No |
0142..0143 | - | - | ProdTest.Reserved_2 | Reserved
0144..014B | - | - | FixedPhoenixNotInRamSection Reserved | Reserved
014C..0150 | FF FF FF FF FF | f | EeVersionHistory |
0151..0155 | FF FF FF FF FF | fs | LockToFp | RFPI to lock when the device is started in testmode.
0156..0157 | 03 FF | f | EepromUsedRfCarriers | Bitfield of carriers which the protocol is allowed to use One bit for each of the 10 carriers.
0158..015D | 7F FF FF FF FF FF | fs | UsedRfCarriers_5g8 | Bitfield of carriers which the protocol is allowed to use One bit for each of the 10 carriers.
015E | 18 | fs | bUSDect8hourHandoverStart | In US/Japan DECT, this value determines when to start handover attempts. One LSB equals 10 min.
015F | 2F | fs | bUSDect8hourHandoverRelease | If handover attempts are not succesfull, a call will terminate after a period determined by the value of this paramter. One LSB equals 10 min. In US/Japan DECT it is only allowed to maintain a channel for a maximum of 8 hours.
0160..016F | FF..FF | fs | DeleteCauseArr | Used by protocol to trace disenrolment.
0170..0174 | FF FF FF FF FF | fs | DeleteRfpi_1 | Used by protocol to trace disenrolment.
0175..0179 | FF FF FF FF FF | fs | DeleteRfpi_2 | Used by protocol to trace disenrolment.
017A..017F |  |  | BmcConfig | BMC configuration
017A | - | - | BmcConfig.S_err | BMC Configuration
017B | - | - | BmcConfig.Slide_Mask | BMC Configuration
017C | - | - | BmcConfig.Vol | BMC Configuration
017D | - | - | BmcConfig.DAC | BMC Configuration
017E | - | - | BmcConfig.WIN | BMC Configuration
017F | - | - | BmcConfig.Enc | BMC Configuration
0180 | 00 | f | default_BMC_CTRL_REG | BMC Configuration
0181 | F0 | f | default_BMC_CTRL2_REG | BMC Configuration
0182 | 32 | fs | HighRssiLimit | Used during enrollment. For the first HighRssiTime seconds of the enrolment only FP s with a rssi higher than HighRssiLimit will be checked if the enroll bit is set.
0183 | 14 | fs | HighRssiTime | See description of HighRssiLimit .
0184 | 00 | f | bNoEmissionModeEnable | Internal parameter for storing the PPs no emission capabilities.
0185..0188 | 00 00 00 00 | fs | bEnrollStatusFlags | Is used to store the status of various CatIq security features. The parameter must only be used by the protocol.
0189..018E | 00 00 00 00 00 00 | fs | bEnrollStatusFlags_Deprecated |
018F..01A2 | - | - | ______EarlyEncryption KeyArr |
018F | - | - | ______EarlyEncryption KeyArr.Element 0.Default CipkerKeyIndexMsb |
0190 | - | - | ______EarlyEncryption KeyArr.Element 0.Default CipkerKeyIndexLsb |
0191..0198 | - | - | ______EarlyEncryption KeyArr.Element 0.Default CipkerKeyArr |
0199 | - | - | ______EarlyEncryption KeyArr.Element 1.Default CipkerKeyIndexMsb |
019A | - | - | ______EarlyEncryption KeyArr.Element 1.Default CipkerKeyIndexLsb |
019B..01A2 | - | - | ______EarlyEncryption KeyArr.Element 1.Default CipkerKeyArr |
01A3 | 08 | f | RfBandgap | Only relevant for LMX4181 based projects - Calibration of the BandGap reference voltage.
01A4 | 00 | f | bProtocolFeatures_Non Shadow |
01A5 | 00 | f | bProtocolFeatures_Non Shadow2 |
01A6..01AA | - | - | RfMacreserved | reserved
Address | Value | Type | Name | Description (Battery Settings)
01AB..01D8 |  |  | HsBatterySettings |
01AB..01AC | - | - | HsBatterySettings.Batt NoVoltage | The voltage at which the handset powers off. Unit = Number of ADC steps on the voltage measurement.
01AD..01AE | - | - | HsBatterySettings.Batt LowVoltage | The voltage at which the user is notified of a low battery. Unit = Number of ADC steps on the voltage measurement.
01AF..01B0 | - | - | HsBatterySettings.Batt HighVoltage | The voltage at which the handset stops charging. Unit = Number of ADC steps on the voltage measurement.
01B1 | - | - | HsBatterySettings.Band GapInit | Note: Not used. Use eep adr 0x006F BandGap in stead.
01B2..01B5 | - | - | HsBatterySettings.Battery Size | The nominal size of the battery. Unit = [10 Ah]
01B6..01B9 | - | - | HsBatterySettings.Estimated Capacity | The Estimated capacity of the battery. Unit = [10 Ah].
01BA | - | - | HsBatterySettings.Batt MaintainChargeTimeout |
01BB | - | - | HsBatterySettings.GoTo FullChargeLevel |
01BC..01BD | - | - | HsBatterySettings.Start MaintainChargeLevel |
01BE | - | - | HsBatterySettings.Temp Coeff |
01BF | - | - | HsBatterySettings.Batt MaxTemperature |
01C0 | - | - | HsBatterySettings.Batt MinTemperature |
01C1..01CA | - | - | HsBatterySettings.Cap Low |
01CB..01D4 | - | - | HsBatterySettings.Cap High |
01D5..01D6 | - | - | HsBatterySettings.SOC ConversionFactor | SOC conversion factor between SOC ticks and estimated capacity ticks . Must be adjusted in production.
01D7..01D8 | - | - | HsBatterySettings.Battery Dummy | Not used.
01D9 | C2 | f | BattTempCoeff |
01DA..01DB | FF FF | f | PatchCodeSrcAddr |
01DC..01DF | FF FF FF FF | f | PatchCodeDstAddr |
Address | Value | Type | Name | Description (Audio)
01E0..022C |  |  | Audio | Audio configuration parameters
01E0 | - | - | Audio.Option | Reserved.
01E1..01F9 |  |  | Audio.Earp | Earpiece audio settings
01E1 | - | - | Audio.Earp.Reserved | Reserved
01E2..01F9 | - | - | Audio.Earp.Vol | Earpiece mode: Volume steps [RxGain, TxGain, SideToneGain]. Unit: dB Range: -128..+127
01E2 | - | - | Audio.Earp.Vol.Element 0.RxGain | Earpiece mode: Volume step 0, receive-gain Unit: dB Range: -128..+127
01E3 | - | - | Audio.Earp.Vol.Element 0.TxGain | Earpiece mode: Volume step 0, transmit-gain Unit: dB Range: -128..+127
01E4 | - | - | Audio.Earp.Vol.Element 0.SideToneGain | Earpiece mode: Volume step 0, sidetone-gain Unit: dB Range: -128..+127
01E5 | - | - | Audio.Earp.Vol.Element 1.RxGain | Earpiece mode: Volume step 1
01E6 | - | - | Audio.Earp.Vol.Element 1.TxGain |
01E7 | - | - | Audio.Earp.Vol.Element 1.SideToneGain |
01E8 | - | - | Audio.Earp.Vol.Element 2.RxGain | Earpiece mode: Volume step 2
01E9 | - | - | Audio.Earp.Vol.Element 2.TxGain |
01EA | - | - | Audio.Earp.Vol.Element 2.SideToneGain |
01EB | - | - | Audio.Earp.Vol.Element 3.RxGain | Earpiece mode: Volume step 3
01EC | - | - | Audio.Earp.Vol.Element 3.TxGain |
01ED | - | - | Audio.Earp.Vol.Element 3.SideToneGain |
01EE | - | - | Audio.Earp.Vol.Element 4.RxGain | Earpiece mode: Volume step 4
01EF | - | - | Audio.Earp.Vol.Element 4.TxGain |
01F0 | - | - | Audio.Earp.Vol.Element 4.SideToneGain |
01F1 | - | - | Audio.Earp.Vol.Element 5.RxGain | Earpiece mode: Volume step 5
01F2 | - | - | Audio.Earp.Vol.Element 5.TxGain |
01F3 | - | - | Audio.Earp.Vol.Element 5.SideToneGain |
01F4 | - | - | Audio.Earp.Vol.Element 6.RxGain |
01F5 | - | - | Audio.Earp.Vol.Element 6.TxGain |
01F6 | - | - | Audio.Earp.Vol.Element 6.SideToneGain |
01F7 | - | - | Audio.Earp.Vol.Element 7.RxGain |
01F8 | - | - | Audio.Earp.Vol.Element 7.TxGain |
01F9 | - | - | Audio.Earp.Vol.Element 7.SideToneGain |
01FA..0212 |  |  | Audio.Heads | Headset audio configuration
01FA | - | - | Audio.Heads.Reserved | Reserved
01FB..0212 | - | - | Audio.Heads.Vol | Headset mode volume steps.
01FB | - | - | Audio.Heads.Vol.Element 0.RxGain | Headset mode: Volume step 0, receive-gain Unit: dB Range: -128..+127
01FC | - | - | Audio.Heads.Vol.Element 0.TxGain | Headset mode: Volume step 0, transmit-gain Unit: dB Range: -128..+127
01FD | - | - | Audio.Heads.Vol.Element 0.SideToneGain | Headset mode: Volume step 0, sidetone-gain Unit: dB Range: -128..+127
01FE | - | - | Audio.Heads.Vol.Element 1.RxGain | Headset mode: Volume step 1
01FF | - | - | Audio.Heads.Vol.Element 1.TxGain |
0200 | - | - | Audio.Heads.Vol.Element 1.SideToneGain |
0201 | - | - | Audio.Heads.Vol.Element 2.RxGain | Headset mode: Volume step 2
0202 | - | - | Audio.Heads.Vol.Element 2.TxGain |
0203 | - | - | Audio.Heads.Vol.Element 2.SideToneGain |
0204 | - | - | Audio.Heads.Vol.Element 3.RxGain | Headset mode: Volume step 3
0205 | - | - | Audio.Heads.Vol.Element 3.TxGain |
0206 | - | - | Audio.Heads.Vol.Element 3.SideToneGain |
0207 | - | - | Audio.Heads.Vol.Element 4.RxGain | Headset mode: Volume step 4
0208 | - | - | Audio.Heads.Vol.Element 4.TxGain |
0209 | - | - | Audio.Heads.Vol.Element 4.SideToneGain |
020A | - | - | Audio.Heads.Vol.Element 5.RxGain | Headset mode: Volume step 5
020B | - | - | Audio.Heads.Vol.Element 5.TxGain |
020C | - | - | Audio.Heads.Vol.Element 5.SideToneGain |
020D | - | - | Audio.Heads.Vol.Element 6.RxGain |
020E | - | - | Audio.Heads.Vol.Element 6.TxGain |
020F | - | - | Audio.Heads.Vol.Element 6.SideToneGain |
0210 | - | - | Audio.Heads.Vol.Element 7.RxGain |
0211 | - | - | Audio.Heads.Vol.Element 7.TxGain |
0212 | - | - | Audio.Heads.Vol.Element 7.SideToneGain |
0213..0223 |  |  | Audio.SpkPh | Speakerphone audio settings
0213 | - | - | Audio.SpkPh.Reserved | Reserved
0214..0223 | - | - | Audio.SpkPh.Vol | Speaker-phone mode: Volume steps [RxGain, TxGain]. Unit: dB Range: -128..+127
0214 | - | - | Audio.SpkPh.Vol.Element 0.RxGain | Speaker-phone mode: Volume step 0, receive-gain Unit: dB Range: -128..+127
0215 | - | - | Audio.SpkPh.Vol.Element 0.TxGain | Speaker-phone mode: Volume step 0, transmit-gain Unit: dB Range: -128..+127
0216 | - | - | Audio.SpkPh.Vol.Element 1.RxGain | Speaker-phone mode: Volume step 1
0217 | - | - | Audio.SpkPh.Vol.Element 1.TxGain |
0218 | - | - | Audio.SpkPh.Vol.Element 2.RxGain | Speaker-phone mode: Volume step 2
0219 | - | - | Audio.SpkPh.Vol.Element 2.TxGain |
021A | - | - | Audio.SpkPh.Vol.Element 3.RxGain | Speaker-phone mode: Volume step 3
021B | - | - | Audio.SpkPh.Vol.Element 3.TxGain |
021C | - | - | Audio.SpkPh.Vol.Element 4.RxGain | Speaker-phone mode: Volume step 4
021D | - | - | Audio.SpkPh.Vol.Element 4.TxGain |
021E | - | - | Audio.SpkPh.Vol.Element 5.RxGain | Speaker-phone mode: Volume step 5
021F | - | - | Audio.SpkPh.Vol.Element 5.TxGain |
0220 | - | - | Audio.SpkPh.Vol.Element 6.RxGain |
0221 | - | - | Audio.SpkPh.Vol.Element 6.TxGain |
0222 | - | - | Audio.SpkPh.Vol.Element 7.RxGain |
0223 | - | - | Audio.SpkPh.Vol.Element 7.TxGain |
0224 | - | - | Audio.MicMuteTime | Timedelay of Mic mute while playing tones Unit: 1ms
0225 | - | - | Audio.CodecPowerUpTime | Time between powering up the codec/external amp. and playing sounds. Unit: 1ms
0226..0227 | - | - | Audio.CodecPowerDownTime | CodecPowerDownTime Time from playing last sound until codec and external amplifier is shutdown. Unit: 1ms
0228..022A |  |  | Audio.CodecAnaAgcCfg | Settings for analog AGC algorithm.
0228 | - | - | Audio.CodecAnaAgcCfg. AnaAgcCLvlMax | Threshold for dec. MIC gain. If this value is greater than or equal to 0 the analog AGC is disabled and normal microphone gain is used. Otherwise analog AGC is enabled. Unit: dB Range: -128dB..127dB Note: See description of AnaAgc in An-d-129 from SiTel for more info.
0229 | - | - | Audio.CodecAnaAgcCfg. AnaAgcCLvlMin | Threshold for inc. MIC gain. Unit: dB Range: -128dB..127dB Note: See description of AnaAgc in An-d-129 from SiTel for more info.
022A | - | - | Audio.CodecAnaAgcCfg. AnaAgcMicMin | Minimum bound for MIC gain. Unit: dB Range: -128dB..127dB Note: See description of AnaAgc in An-d-129 from SiTel for more info.
022B..022C | - | - | Audio.Reserved | Reserved
Address | Value | Type | Name | Description (Audio Unit - CODEC)
022D..033B |  |  | AudioUnit | Audio codec configuration
022D | - | - | AudioUnit.Codec.Cfg.Flags | MIC and SPK-filter parameter-set selection
022D | - | - | AudioUnit.Codec.Cfg.Flags. pset_micfilt | MIC-filter parameter set selection. 0=use eeprom settings 1=bypass 2=use code-const settings
022D | - | - | AudioUnit.Codec.Cfg.Flags. pset_spkfilt | SPK-filter parameter set selection. 0=use eeprom settings 1=bypass 2=use code-const settings
022E..022F | - | - | AudioUnit.Codec.NC100 Hz8KhzCfg.alpha | Non-silent convergence parameter (recommended value = 0x1000 - 0x7FFF)
0230..0231 | - | - | AudioUnit.Codec.NC100 Hz8KhzCfg.beta | Silent convergence parameter (recommended value = 0x0000 - 0x0008)
0232..0233 | - | - | AudioUnit.Codec.NC100 Hz8KhzCfg.threshold | Amplitude threshold for silence (recommended value = 0x0040)
0234..0235 | - | - | AudioUnit.Codec.NC100 Hz16KhzCfg.alpha | Non-silent convergence parameter (recommended value = 0x1000 - 0x7FFF)
0236..0237 | - | - | AudioUnit.Codec.NC100 Hz16KhzCfg.beta | Silent convergence parameter (recommended value = 0x0000 - 0x0008)
0238..0239 | - | - | AudioUnit.Codec.NC100 Hz16KhzCfg.threshold | Amplitude threshold for silence (recommended value = 0x0040)
023A..0255 |  |  | AudioUnit.Codec.Set_8 Khz.SpkFilt_Earp | Earpiece-mode/8Khz. Speaker-filters Pfilt1 and Pfilt2 parameters.
023A..0247 |  |  | AudioUnit.Codec.Set_8 Khz.SpkFilt_Earp.PFilt1 | Earpiece-mode/8Khz. Speaker-filters Pfilt1 parameters.
023A..023B | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Earp.PFilt1. C0 | PFILT parameter C0, coefficient
023C..023D | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Earp.PFilt1. C1 | PFILT parameter C1, coefficient
023E..023F | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Earp.PFilt1. C2 | PFILT parameter C2, coefficient
0240..0241 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Earp.PFilt1. C3 | PFILT parameter C3, coefficient
0242..0243 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Earp.PFilt1. C4 | PFILT parameter C4, coefficient
0244..0245 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Earp.PFilt1. Fin_Att | PFILT parameter Fin_Att, input attenuation. Unit: Q15 Range: 0..7FFF
0246..0247 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Earp.PFilt1. Foutgains | PFILT parameter outgains, output gain and coefficient scaling
0248..0255 |  |  | AudioUnit.Codec.Set_8 Khz.SpkFilt_Earp.PFilt2 | Earpiece-mode/8Khz. Speaker-filters Pfilt2 parameters.
0248..0249 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Earp.PFilt2. C0 | PFILT parameter C0, coefficient
024A..024B | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Earp.PFilt2. C1 | PFILT parameter C1, coefficient
024C..024D | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Earp.PFilt2. C2 | PFILT parameter C2, coefficient
024E..024F | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Earp.PFilt2. C3 | PFILT parameter C3, coefficient
0250..0251 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Earp.PFilt2. C4 | PFILT parameter C4, coefficient
0252..0253 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Earp.PFilt2. Fin_Att | PFILT parameter Fin_Att, input attenuation.
0254..0255 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Earp.PFilt2. Foutgains | PFILT parameter outgains, output gain and coefficient scaling
0256..0271 |  |  | AudioUnit.Codec.Set_8 Khz.SpkFilt_Headset | Headset mode/8khz. Speaker-filter Pfilt1 and Pfilt2 parameters
0256..0263 |  |  | AudioUnit.Codec.Set_8 Khz.SpkFilt_Headset.P Filt1 | Headset mode/8khz. Speaker-filter Pfilt1 parameters
0256..0257 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Headset.P Filt1.C0 | PFILT parameter C0, coefficient
0258..0259 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Headset.P Filt1.C1 | PFILT parameter C1, coefficient
025A..025B | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Headset.P Filt1.C2 | PFILT parameter C2, coefficient
025C..025D | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Headset.P Filt1.C3 | PFILT parameter C3, coefficient
025E..025F | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Headset.P Filt1.C4 | PFILT parameter C4, coefficient
0260..0261 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Headset.P Filt1.Fin_Att | PFILT parameter Fin_Att, input attenuation.
0262..0263 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Headset.P Filt1.Foutgains | PFILT parameter outgains, output gain and coefficient scaling
0264..0271 |  |  | AudioUnit.Codec.Set_8 Khz.SpkFilt_Headset.P Filt2 | Headset mode/8khz. Speaker-filter Pfilt2 parameters
0264..0265 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Headset.P Filt2.C0 | PFILT parameter C0, coefficient
0266..0267 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Headset.P Filt2.C1 | PFILT parameter C1, coefficient
0268..0269 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Headset.P Filt2.C2 | PFILT parameter C2, coefficient
026A..026B | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Headset.P Filt2.C3 | PFILT parameter C3, coefficient
026C..026D | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Headset.P Filt2.C4 | PFILT parameter C4, coefficient
026E..026F | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Headset.P Filt2.Fin_Att | PFILT parameter Fin_Att, input attenuation.
0270..0271 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_Headset.P Filt2.Foutgains | PFILT parameter outgains, output gain and coefficient scaling
0272..028D |  |  | AudioUnit.Codec.Set_8 Khz.SpkFilt_SpkPh | Speaker phone mode/8khz. Speaker-filter Pfilt1 and Pfilt2 parameters
0272..027F |  |  | AudioUnit.Codec.Set_8 Khz.SpkFilt_SpkPh.PFilt1 | Speaker-Phone mode/8khz. Speaker-filter Pfilt1 parameters
0272..0273 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_SpkPh.PFilt1. C0 | PFILT parameter C0, coefficient
0274..0275 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_SpkPh.PFilt1. C1 | PFILT parameter C1, coefficient
0276..0277 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_SpkPh.PFilt1. C2 | PFILT parameter C2, coefficient
0278..0279 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_SpkPh.PFilt1. C3 | PFILT parameter C3, coefficient
027A..027B | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_SpkPh.PFilt1. C4 | PFILT parameter C4, coefficient
027C..027D | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_SpkPh.PFilt1. Fin_Att | PFILT parameter Fin_Att, input attenuation.
027E..027F | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_SpkPh.PFilt1. Foutgains | PFILT parameter outgains, output gain and coefficient scaling
0280..028D |  |  | AudioUnit.Codec.Set_8 Khz.SpkFilt_SpkPh.PFilt2 | Speaker-Phone mode/8khz. Speaker-filter Pfilt2 parameters
0280..0281 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_SpkPh.PFilt2. C0 | PFILT parameter C0, coefficient
0282..0283 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_SpkPh.PFilt2. C1 | PFILT parameter C1, coefficient
0284..0285 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_SpkPh.PFilt2. C2 | PFILT parameter C2, coefficient
0286..0287 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_SpkPh.PFilt2. C3 | PFILT parameter C3, coefficient
0288..0289 | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_SpkPh.PFilt2. C4 | PFILT parameter C4, coefficient
028A..028B | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_SpkPh.PFilt2. Fin_Att | PFILT parameter Fin_Att, input attenuation.
028C..028D | - | - | AudioUnit.Codec.Set_8 Khz.SpkFilt_SpkPh.PFilt2. Foutgains | PFILT parameter outgains, output gain and coefficient scaling
028E..02A9 |  |  | AudioUnit.Codec.Set_8 Khz.MicFilt | Common/8khz. Mic-filter pfilt3 and pfilt4 coefficients
028E..029B |  |  | AudioUnit.Codec.Set_8 Khz.MicFilt.PFilt3 | Common MIC-filter Pfilt3 parameters.
028E..028F | - | - | AudioUnit.Codec.Set_8 Khz.MicFilt.PFilt3.C0 | PFILT parameter C0, coefficient
0290..0291 | - | - | AudioUnit.Codec.Set_8 Khz.MicFilt.PFilt3.C1 | PFILT parameter C1, coefficient
0292..0293 | - | - | AudioUnit.Codec.Set_8 Khz.MicFilt.PFilt3.C2 | PFILT parameter C2, coefficient
0294..0295 | - | - | AudioUnit.Codec.Set_8 Khz.MicFilt.PFilt3.C3 | PFILT parameter C3, coefficient
0296..0297 | - | - | AudioUnit.Codec.Set_8 Khz.MicFilt.PFilt3.C4 | PFILT parameter C4, coefficient
0298..0299 | - | - | AudioUnit.Codec.Set_8 Khz.MicFilt.PFilt3.Fin_ Att | PFILT parameter Fin_Att, input attenuation.
029A..029B | - | - | AudioUnit.Codec.Set_8 Khz.MicFilt.PFilt3.Foutgains | PFILT parameter outgains, output gain and coefficient scaling
029C..02A9 |  |  | AudioUnit.Codec.Set_8 Khz.MicFilt.PFilt4 | Common MIC-filter Pfilt4 parameters.
029C..029D | - | - | AudioUnit.Codec.Set_8 Khz.MicFilt.PFilt4.C0 | PFILT parameter C0, coefficient
029E..029F | - | - | AudioUnit.Codec.Set_8 Khz.MicFilt.PFilt4.C1 | PFILT parameter C1, coefficient
02A0..02A1 | - | - | AudioUnit.Codec.Set_8 Khz.MicFilt.PFilt4.C2 | PFILT parameter C2, coefficient
02A2..02A3 | - | - | AudioUnit.Codec.Set_8 Khz.MicFilt.PFilt4.C3 | PFILT parameter C3, coefficient
02A4..02A5 | - | - | AudioUnit.Codec.Set_8 Khz.MicFilt.PFilt4.C4 | PFILT parameter C4, coefficient
02A6..02A7 | - | - | AudioUnit.Codec.Set_8 Khz.MicFilt.PFilt4.Fin_ Att | PFILT parameter Fin_Att, input attenuation.
02A8..02A9 | - | - | AudioUnit.Codec.Set_8 Khz.MicFilt.PFilt4.Foutgains | PFILT parameter outgains, output gain and coefficient scaling
02AA..02C5 |  |  | AudioUnit.Codec.Set_16 Khz.SpkFilt_Earp | Earpiece-mode/16Khz. Speaker-filters Pfilt1 and Pfilt2 parameters. Same layout as for 8 kHz.
02AA..02B7 |  |  | AudioUnit.Codec.Set_16 Khz.SpkFilt_Earp.PFilt1 | Earpiece-mode/16Khz. Speaker-filters Pfilt1 parameters
02AA..02AB | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Earp.PFilt1. C0 |
02AC..02AD | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Earp.PFilt1. C1 |
02AE..02AF | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Earp.PFilt1. C2 |
02B0..02B1 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Earp.PFilt1. C3 |
02B2..02B3 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Earp.PFilt1. C4 |
02B4..02B5 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Earp.PFilt1. Fin_Att |
02B6..02B7 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Earp.PFilt1. Foutgains |
02B8..02C5 |  |  | AudioUnit.Codec.Set_16 Khz.SpkFilt_Earp.PFilt2 | Earpiece-mode/16Khz. Speaker-filters Pfilt2 parameters
02B8..02B9 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Earp.PFilt2. C0 |
02BA..02BB | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Earp.PFilt2. C1 |
02BC..02BD | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Earp.PFilt2. C2 |
02BE..02BF | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Earp.PFilt2. C3 |
02C0..02C1 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Earp.PFilt2. C4 |
02C2..02C3 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Earp.PFilt2. Fin_Att |
02C4..02C5 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Earp.PFilt2. Foutgains |
02C6..02E1 |  |  | AudioUnit.Codec.Set_16 Khz.SpkFilt_Headset | Headset mode/16khz. Speaker-filter Pfilt1 and Pfilt2 parameters. Same layout as 8 kHz.
02C6..02D3 |  |  | AudioUnit.Codec.Set_16 Khz.SpkFilt_Headset.P Filt1 | Headset mode/16khz. Speaker-filter Pfilt1 parameters. Same layout as 8 kHz.
02C6..02C7 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Headset.P Filt1.C0 |
02C8..02C9 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Headset.P Filt1.C1 |
02CA..02CB | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Headset.P Filt1.C2 |
02CC..02CD | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Headset.P Filt1.C3 |
02CE..02CF | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Headset.P Filt1.C4 |
02D0..02D1 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Headset.P Filt1.Fin_Att |
02D2..02D3 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Headset.P Filt1.Foutgains |
02D4..02E1 |  |  | AudioUnit.Codec.Set_16 Khz.SpkFilt_Headset.P Filt2 | Headset mode/16khz. Speaker-filter Pfilt2 parameters. Same layout as 8 kHz.
02D4..02D5 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Headset.P Filt2.C0 |
02D6..02D7 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Headset.P Filt2.C1 |
02D8..02D9 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Headset.P Filt2.C2 |
02DA..02DB | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Headset.P Filt2.C3 |
02DC..02DD | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Headset.P Filt2.C4 |
02DE..02DF | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Headset.P Filt2.Fin_Att |
02E0..02E1 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_Headset.P Filt2.Foutgains |
02E2..02FD |  |  | AudioUnit.Codec.Set_16 Khz.SpkFilt_SpkPh | Speaker-phone mode/16khz. Speaker-filter Pfilt1 and Pfilt2 parameters. Same layout as 8 kHz.
02E2..02EF |  |  | AudioUnit.Codec.Set_16 Khz.SpkFilt_SpkPh.PFilt1 | Speaker-phone mode/16khz. Speaker-filter Pfilt1 parameters. Same layout as 8 kHz.
02E2..02E3 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_SpkPh.PFilt1. C0 |
02E4..02E5 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_SpkPh.PFilt1. C1 |
02E6..02E7 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_SpkPh.PFilt1. C2 |
02E8..02E9 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_SpkPh.PFilt1. C3 |
02EA..02EB | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_SpkPh.PFilt1. C4 |
02EC..02ED | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_SpkPh.PFilt1. Fin_Att |
02EE..02EF | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_SpkPh.PFilt1. Foutgains |
02F0..02FD |  |  | AudioUnit.Codec.Set_16 Khz.SpkFilt_SpkPh.PFilt2 | Speaker-phone mode/16khz. Speaker-filter Pfilt2 parameters. Same layout as 8 kHz.
02F0..02F1 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_SpkPh.PFilt2. C0 |
02F2..02F3 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_SpkPh.PFilt2. C1 |
02F4..02F5 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_SpkPh.PFilt2. C2 |
02F6..02F7 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_SpkPh.PFilt2. C3 |
02F8..02F9 | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_SpkPh.PFilt2. C4 |
02FA..02FB | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_SpkPh.PFilt2. Fin_Att |
02FC..02FD | - | - | AudioUnit.Codec.Set_16 Khz.SpkFilt_SpkPh.PFilt2. Foutgains |
02FE..0319 |  |  | AudioUnit.Codec.Set_16 Khz.MicFilt | Common/16khz. Mic-filter pfilt3 and pfilt4 coefficients. Same layout as 8 kHz.
02FE..030B |  |  | AudioUnit.Codec.Set_16 Khz.MicFilt.PFilt3 | Common/16khz. Mic-filter pfilt3 coefficients. Same layout as 8 kHz.
02FE..02FF | - | - | AudioUnit.Codec.Set_16 Khz.MicFilt.PFilt3.C0 |
0300..0301 | - | - | AudioUnit.Codec.Set_16 Khz.MicFilt.PFilt3.C1 |
0302..0303 | - | - | AudioUnit.Codec.Set_16 Khz.MicFilt.PFilt3.C2 |
0304..0305 | - | - | AudioUnit.Codec.Set_16 Khz.MicFilt.PFilt3.C3 |
0306..0307 | - | - | AudioUnit.Codec.Set_16 Khz.MicFilt.PFilt3.C4 |
0308..0309 | - | - | AudioUnit.Codec.Set_16 Khz.MicFilt.PFilt3.Fin_ Att |
030A..030B | - | - | AudioUnit.Codec.Set_16 Khz.MicFilt.PFilt3.Foutgains |
030C..0319 |  |  | AudioUnit.Codec.Set_16 Khz.MicFilt.PFilt4 | Common/16khz. Mic-filter pfilt4 coefficients. Same layout as 8 kHz.
030C..030D | - | - | AudioUnit.Codec.Set_16 Khz.MicFilt.PFilt4.C0 |
030E..030F | - | - | AudioUnit.Codec.Set_16 Khz.MicFilt.PFilt4.C1 |
0310..0311 | - | - | AudioUnit.Codec.Set_16 Khz.MicFilt.PFilt4.C2 |
0312..0313 | - | - | AudioUnit.Codec.Set_16 Khz.MicFilt.PFilt4.C3 |
0314..0315 | - | - | AudioUnit.Codec.Set_16 Khz.MicFilt.PFilt4.C4 |
0316..0317 | - | - | AudioUnit.Codec.Set_16 Khz.MicFilt.PFilt4.Fin_ Att |
0318..0319 | - | - | AudioUnit.Codec.Set_16 Khz.MicFilt.PFilt4.Foutgains |
031A..031B | - | - | AudioUnit.Codec.VolCtrl Cfg.AgcThresholdLvl | Threshold for Limiter in VolCtrl block. Range: 0x0000 - 0x7FFF
031C..031D | - | - | AudioUnit.Codec.VolCtrl Cfg.Supp_centclip_att | NA
031E..031F | - | - | AudioUnit.Codec.VolCtrl Cfg.Supp_centclip | NA
0320..0321 | - | - | AudioUnit.Codec.MicPost Cfg.Supp_centclip_att | Maximum attenuation in Tx Noise Gate. Range: 0x0000 - 0x7FFF
0322..0323 | - | - | AudioUnit.Codec.MicPost Cfg.Supp_centclip | Threshold level for Tx Noise Gate - input signal must be below this to start attenuation. Range: 0x0000 - 0x7FFF
0324..032E | - | - | AudioUnit.ReservedHfree | Reserved
032F..0330 | - | - | AudioUnit.EcUnit.Lec_ Ratio2 | Decision for using u0 or u1/2/3. Note: See An-d-129 from Dialog for description of parameter.
0331..0332 | - | - | AudioUnit.EcUnit.Supp_ On_8kHz | Suppressor on parameter for specifying the amount of attenuation when suppressor is active. Depends on the rbetaon time constant. Note: See An-d-129 from Dialog for description of parameter.
0333..0334 | - | - | AudioUnit.EcUnit.Supp_ On_16kHz | Suppressor on parameter for specifying the amount of attenuation when suppressor is active. Depends on the rbetaon time constant. Note: See An-d-129 from Dialog for description of parameter.
0335 | - | - | AudioUnit.Reservedb | Reserved
0336..033B | - | - | AudioUnit.Reserved | Reserved
033C..0365 |  |  | AudioUnitPaec.Paec |
Address | Value | Type | Name | Description (Audio Unit - PAEC)
033C..033D | - | - | AudioUnitPaec.Paec.Paec Cfg_8kHz.cctc | Time constant for the coloration effect filter (cross correlation and auto correlations) Note: See An-d-162 from Dialog for description of parameter.
033E..033F | - | - | AudioUnitPaec.Paec.Paec Cfg_8kHz.smoothdef | Gain Filter Smoothing control Rx mode time constant. Note: See An-d-162 from Dialog for description of parameter.
0340..0341 | - | - | AudioUnitPaec.Paec.Paec Cfg_8kHz.smoothlow | Note: See An-d-162 from Dialog for description of parameter.
0342..0343 | - | - | AudioUnitPaec.Paec.Paec Cfg_8kHz.smoothtop | Gain Filter Smoothing control Doubletalk mode time constant 1. Controls suppression time of room echo tail. Note: See An-d-162 from Dialog for description of parameter.
0344..0345 | - | - | AudioUnitPaec.Paec.Paec Cfg_16kHz.cctc | Time constant for the coloration effect filter (cross correlation and auto correlations) Note: See An-d-162 from Dialog for description of parameter.
0346..0347 | - | - | AudioUnitPaec.Paec.Paec Cfg_16kHz.smoothdef | Gain Filter Smoothing control Rx mode time constant. Note: See An-d-162 from Dialog for description of parameter.
0348..0349 | - | - | AudioUnitPaec.Paec.Paec Cfg_16kHz.smoothlow | Gain Filter Smoothing control Doubletalk mode time constant 1. Controls suppression time of room echo tail. Note: See An-d-162 from Dialog for description of parameter.
034A..034B | - | - | AudioUnitPaec.Paec.Paec Cfg_16kHz.smoothtop | Gain Filter Smoothing control Doubletalk mode time constant 2. Controls capture of early room echoes. Note: See An-d-162 from Dialog for description of parameter.
034C..034D | - | - | AudioUnitPaec.Paec.Paec Cfg.init | Number of frames with initial fast convergence time constants, multiplied with -1. Note: See An-d-162 from Dialog for description of parameter.
034E..034F | - | - | AudioUnitPaec.Paec.Paec Cfg.noiseestgainshft | Tx noise level estimation scaling factor. Note: See An-d-162 from Dialog for description of parameter.
0350..0351 | - | - | AudioUnitPaec.Paec.Paec Cfg.noiseestspkgainshft | Rx noise level estimation scaling factor. Note: See An-d-162 from Dialog for description of parameter.
0352..0353 | - | - | AudioUnitPaec.Paec.Paec Cfg.gamma | Scaling parameter of the echo removal filter. Note: See An-d-162 from Dialog for description of parameter.
0354..0355 | - | - | AudioUnitPaec.Paec.Paec Cfg.beta | Gain given to echo estimate to avoid under-estimation. Note: See An-d-162 from Dialog for description of parameter.
0356..0357 | - | - | AudioUnitPaec.Paec.Paec Cfg.attlimit | Attenuation Limit (application dependant). Note: See An-d-162 from Dialog for description of parameter.
0358..0359 | - | - | AudioUnitPaec.Paec.Paec Cfg.noiseattlimit | Noise Suppression attenuation factor (0..-10dB). Note: See An-d-162 from Dialog for description of parameter.
035A..035B | - | - | AudioUnitPaec.Paec.Paec Cfg.retainnoisethr1div | Rx noise retaining threshold. Note: See An-d-162 from Dialog for description of parameter.
035C..035D | - | - | AudioUnitPaec.Paec.Paec Cfg.attlimitthr1div | Attenuation limit minimum threshold. Note: See An-d-162 from Dialog for description of parameter.
035E..035F | - | - | AudioUnitPaec.Paec.Paec Cfg.smooththr | Gain Filter Smoothing control threshold. Note: See An-d-162 from Dialog for description of parameter.
0360..0361 | - | - | AudioUnitPaec.Paec.Paec Cfg.extra_shift | Additional shift for internal scaling. Note: See An-d-162 from Dialog for description of parameter.
0362..0363 | - | - | AudioUnitPaec.Paec.Paec Cfg.intshift_maxnorm | Headroom for internal dynamic scaling (16 - no of bits). Note: See An-d-162 from Dialog for description of parameter.
0364 | - | - | AudioUnitPaec.Paec.Paec Cfg.txgain | This parameter is a dB setting og the tx-gain after the PAEC. So it is a post-PAEC gain of the microphone signal. Unit: dB Range: -128..+127 Note: See An-d-162 from Dialog for description of parameter.
0365 | - | - | AudioUnitPaec.Paec.reserved | Reserved
Address | Value | Type | Name | Description (Subscriptions)
0366..038C |  |  | Subs0 | Subscription 0.
0366..036A | FF FF FF FF FF | fs | Subs0.RFPI | RFPI for subscription0
036B | FF | fs | Subs0.ServiceClass | ServiceClass for subscription0
036C | FF | fs | Subs0.LAL | LAL for subscription0
036D | FF | fs | Subs0.IpuiLen | IPUI length for subscription0
036E..037A | FF..FF | fs | Subs0.IPUI | IPUI for subscription0
037B | FF | fs | Subs0.ZAP | ZAP for subscription0
037C | FF | fs | Subs0.Status | Status for subscription0
037D..038C | FF..FF | fs | Subs0.UAK | UAK for subscription0
038D..03B3 |  |  | Subs1 | Subscription 1. (Same structure as Subs0).
038D..0391 | FF FF FF FF FF | fs | Subs1.RFPI |
0392 | FF | fs | Subs1.ServiceClass |
0393 | FF | fs | Subs1.LAL |
0394 | FF | fs | Subs1.IpuiLen |
0395..03A1 | FF..FF | fs | Subs1.IPUI |
03A2 | FF | fs | Subs1.ZAP |
03A3 | FF | fs | Subs1.Status |
03A4..03B3 | FF..FF | fs | Subs1.UAK |
03B4..03DA |  |  | Subs2 | Subscription 2. (Same structure as Subs0).
03B4..03B8 | FF FF FF FF FF | fs | Subs2.RFPI |
03B9 | FF | fs | Subs2.ServiceClass |
03BA | FF | fs | Subs2.LAL |
03BB | FF | fs | Subs2.IpuiLen |
03BC..03C8 | FF..FF | fs | Subs2.IPUI |
03C9 | FF | fs | Subs2.ZAP |
03CA | FF | fs | Subs2.Status |
03CB..03DA | FF..FF | fs | Subs2.UAK |
03DB..0401 |  |  | Subs3 | Subscription 3. (Same structure as Subs0).
03DB..03DF | FF FF FF FF FF | fs | Subs3.RFPI |
03E0 | FF | fs | Subs3.ServiceClass |
03E1 | FF | fs | Subs3.LAL |
03E2 | FF | fs | Subs3.IpuiLen |
03E3..03EF | FF..FF | fs | Subs3.IPUI |
03F0 | FF | fs | Subs3.ZAP |
03F1 | FF | fs | Subs3.Status |
03F2..0401 | FF..FF | fs | Subs3.UAK |
0402..04EB | FF..FF | fs | Subs49_Deprecated |
0402..0406 | FF FF FF FF FF | fs | Subs49_Deprecated.Element 0.RFPI |
0407 | FF | fs | Subs49_Deprecated.Element 0.ServiceClass |
0408 | FF | fs | Subs49_Deprecated.Element 0.LAL |
0409 | FF | fs | Subs49_Deprecated.Element 0.IpuiLen |
040A..0416 | FF..FF | fs | Subs49_Deprecated.Element 0.IPUI |
0417 | FF | fs | Subs49_Deprecated.Element 0.ZAP |
0418 | FF | fs | Subs49_Deprecated.Element 0.Status |
0419..0428 | FF..FF | fs | Subs49_Deprecated.Element 0.UAK |
0429..042D | FF FF FF FF FF | fs | Subs49_Deprecated.Element 1.RFPI |
042E | FF | fs | Subs49_Deprecated.Element 1.ServiceClass |
042F | FF | fs | Subs49_Deprecated.Element 1.LAL |
0430 | FF | fs | Subs49_Deprecated.Element 1.IpuiLen |
0431..043D | FF..FF | fs | Subs49_Deprecated.Element 1.IPUI |
043E | FF | fs | Subs49_Deprecated.Element 1.ZAP |
043F | FF | fs | Subs49_Deprecated.Element 1.Status |
0440..044F | FF..FF | fs | Subs49_Deprecated.Element 1.UAK |
0450..0454 | FF FF FF FF FF | fs | Subs49_Deprecated.Element 2.RFPI |
0455 | FF | fs | Subs49_Deprecated.Element 2.ServiceClass |
0456 | FF | fs | Subs49_Deprecated.Element 2.LAL |
0457 | FF | fs | Subs49_Deprecated.Element 2.IpuiLen |
0458..0464 | FF..FF | fs | Subs49_Deprecated.Element 2.IPUI |
0465 | FF | fs | Subs49_Deprecated.Element 2.ZAP |
0466 | FF | fs | Subs49_Deprecated.Element 2.Status |
0467..0476 | FF..FF | fs | Subs49_Deprecated.Element 2.UAK |
0477..047B | FF FF FF FF FF | fs | Subs49_Deprecated.Element 3.RFPI |
047C | FF | fs | Subs49_Deprecated.Element 3.ServiceClass |
047D | FF | fs | Subs49_Deprecated.Element 3.LAL |
047E | FF | fs | Subs49_Deprecated.Element 3.IpuiLen |
047F..048B | FF..FF | fs | Subs49_Deprecated.Element 3.IPUI |
048C | FF | fs | Subs49_Deprecated.Element 3.ZAP |
048D | FF | fs | Subs49_Deprecated.Element 3.Status |
048E..049D | FF..FF | fs | Subs49_Deprecated.Element 3.UAK |
049E..04A2 | FF FF FF FF FF | fs | Subs49_Deprecated.Element 4.RFPI |
04A3 | FF | fs | Subs49_Deprecated.Element 4.ServiceClass |
04A4 | FF | fs | Subs49_Deprecated.Element 4.LAL |
04A5 | FF | fs | Subs49_Deprecated.Element 4.IpuiLen |
04A6..04B2 | FF..FF | fs | Subs49_Deprecated.Element 4.IPUI |
04B3 | FF | fs | Subs49_Deprecated.Element 4.ZAP |
04B4 | FF | fs | Subs49_Deprecated.Element 4.Status |
04B5..04C4 | FF..FF | fs | Subs49_Deprecated.Element 4.UAK |
04C5..04C9 | FF FF FF FF FF | fs | Subs49_Deprecated.Element 5.RFPI |
04CA | FF | fs | Subs49_Deprecated.Element 5.ServiceClass |
04CB | FF | fs | Subs49_Deprecated.Element 5.LAL |
04CC | FF | fs | Subs49_Deprecated.Element 5.IpuiLen |
04CD..04D9 | FF..FF | fs | Subs49_Deprecated.Element 5.IPUI |
04DA | FF | fs | Subs49_Deprecated.Element 5.ZAP |
04DB | FF | fs | Subs49_Deprecated.Element 5.Status |
04DC..04EB | FF..FF | fs | Subs49_Deprecated.Element 5.UAK |
04EC | FF | fs | FwuMode |
04ED | 00 | fs | CustomFixes |
04EE..04EF | - | - | FwuCrc |
04F0..04F3 | - | - | FwuStartOffset |
04F4 | 60 | fs | Provider |
04F5 | 00 | f | CurrentVariantId |
04F6 | 08 | fs | PeriodicLocationTime |
04F7 | 01 | fs | PeriodicLocationDefined TimeLimit |
04F8 | - | - | EncStartCheckTime | The feature checks if encryption is enabled EncStartCheckTime seconds after the call is connected. If the encryption is not started, then the mail PP_MAC_ENC_NOT_STARTED is send to USER_TASK. The feature is obsolete, because there is now a similar CatIq feature.
04F9..04FC | 00 00 00 00 | f | FinalTest |
04F9..04FC | 00 00 00 00 | f | FinalTest.AllTests |
04F9..04FC |  |  | FinalTest.struct |
04F9 | xxxxxxx0 | f | FinalTest.struct.Display |
04F9 | xxxxxx0x | f | FinalTest.struct.Keyboard |
04F9 | xxxxx0xx | f | FinalTest.struct.Backlight |
04F9 | xxxx0xxx | f | FinalTest.struct.LEDIndicator |
04F9 | xxx0xxxx | f | FinalTest.struct.Vibrator |
04F9 | xx0xxxxx | f | FinalTest.struct.Battery |
04F9 | x0xxxxxx | f | FinalTest.struct.Earpiece Tone |
04F9 | 0xxxxxxx | f | FinalTest.struct.Speaker Tone |
04FA | xxxxxxx0 | f | FinalTest.struct.Headset Tone |
04FA | xxxxxx0x | f | FinalTest.struct.Loop Audio |
04FA | xxxxx0xx | f | FinalTest.struct.Loop AudioSpeaker |
04FA | xxxx0xxx | f | FinalTest.struct.SdCard |
04FA | xxx0xxxx | f | FinalTest.struct.Bluetooth |
04FA | xx0xxxxx | f | FinalTest.struct.Noise Reduction |
04FA | x0xxxxxx | f | FinalTest.struct.Pull Cord |
04FA | 0xxxxxxx | f | FinalTest.struct.ManDown |
04FB | xxxxxxx0 | f | FinalTest.struct.SwInfo |
04FB | xxxxxx0x | f | FinalTest.struct.Dect Mode |
04FB | xxxxx0xx | f | FinalTest.struct.Prod Data |
04FB | xxxx0xxx | f | FinalTest.struct.Provider |
04FB | xxx0xxxx | f | FinalTest.struct.Eeprom |
04FB | xx0xxxxx | f | FinalTest.struct.Loop AudioEarpiece |
04FB | 00xxxxxx | f | FinalTest.struct.Reserved | Reserved
04FC | 00000000 | f | FinalTest.struct.Reserved2 | Reserved
04FD..0501 | FF FF FF FF FF | fs5 | FactTestIpeiBackup |
0502 | - | - | HwVersion |
0503 | 60 | fs | MmiProvider |
0504 | 00 | f | TestInitialize |
0505..050A | 00 00 00 00 00 00 | f | Deprecated_TestIoEeprom |
050B..0513 | - | - | Reserved | Reserved
0514..0519 |  |  | Deprecated_HeadsetCtrl |
0514..0515 | - | - | Deprecated_HeadsetCtrl. ThresholdIdle |
0516..0517 | - | - | Deprecated_HeadsetCtrl. ThresholdHook |
0518..0519 | - | - | Deprecated_HeadsetCtrl. ThresholdInCall |
051A | - | - | FwuOptions |
051B..051F | - | - | FwuLoaderStatus |
0520..0528 | - | - | Reserved_FwuSettings1 | Reserved
0529..052A | - | - | FwuNextWriteBlock |
Address | Value | Type | Name | Description (Protected Settings)
052B..052F | 30 30 30 30 00 | fs | SecurityPin | Security Pin. Unit: Chars
0530 | FF | fs1 | Deprecated_ProMenuFlags |
0531..0538 | FF FF FF FF FF FF FF FF | fs1 | Deprecated_ProtectedSetting | Protected Setting Flags. See description of the individual flags below.
0539..053A | FF FF | fs1 | Deprecated_ProtectedSetting2 | Deprecated_ProtectedSetting2 Flags. See description of the individual flags below.
053B..0540 | - | - | MainMenuShortcutTable | Main menu icon shortcuts. Note: See NaviKeyShortcut description of range and values
0541 | - | - | unused1 |
0542..0543 |  |  | KeyBoardPWM |
0542 | - | - | KeyBoardPWM.OnPWM |
0542 | - | - | KeyBoardPWM.DimPWM |
0543 | - | - | KeyBoardPWM.OnCP |
0543 | - | - | KeyBoardPWM.DimCP |
0543 | - | - | KeyBoardPWM.EnablePWM |
0543 | - | - | KeyBoardPWM.reserved |
0544..0545 |  |  | DisplayPWM |
0544 | - | - | DisplayPWM.OnPWM |
0544 | - | - | DisplayPWM.DimPWM |
0545 | - | - | DisplayPWM.OnCP |
0545 | - | - | DisplayPWM.DimCP |
0545 | - | - | DisplayPWM.EnablePWM |
0545 | - | - | DisplayPWM.reserved |
Address | Value | Type | Name | Description (Audio Settings)
0546..0548 |  |  | AudioUserSettings | Audio Settings. See the description of the individual elements below.
0546 | 03 | fs4 | AudioUserSettings.Headset Volume | Headset Volume. Range: 0..7
0547 | 03 | fs4 | AudioUserSettings.Speaker Volume | Speaker Volume. Range: 0..7
0548 | 03 | fs4 | AudioUserSettings.Earpiece Volume | Earpiece Volume. Range: 0..7
0549..0554 |  |  | AudioSettings |
0549..054D | - | - | AudioSettings.AudioVolume StepInDb |
054E..0554 |  |  | AudioSettings.ToneVolume InDb |
054E | E5 | fs4 | AudioSettings.ToneVolume InDb.GeneralVol |
054F | E5 | fs4 | AudioSettings.ToneVolume InDb.OkVol |
0550 | F0 | fs4 | AudioSettings.ToneVolume InDb.ErrorVol |
0551 | E5 | fs4 | AudioSettings.ToneVolume InDb.CradleVol |
0552 | F0 | fs4 | AudioSettings.ToneVolume InDb.KeyPressVol |
0553 | E5 | fs4 | AudioSettings.ToneVolume InDb.RangeVol |
0554 | E5 | fs4 | AudioSettings.ToneVolume InDb.CallWaitVol |
0555 | 00 | fs4 | AudioFlags |
0555 | 00000000 | fs4 | AudioFlags.unused |
0556 | 00 | fs4 | AGCEnabled |
0557 | - | - | unused2 |
Address | Value | Type | Name | Description (General Settings)
0558..0574 |  |  | GeneralSettings | General Settings. See the description of the individual elements below.
0558 | - | - | GeneralSettings.Language | Language. Note: Some languages are not in use on this platform, which is why the list is not continous. Setting this field to other values than defined below will result in undefined behaviour. 0x00=English 0x01=Spanish 0x02=German 0x03=French 0x04=Italian 0x05=Dutch 0x06=Portuguese 0x07=Danish 0x08=Swedish 0x0E=Norwegian 0x13=Finnish Range: 0..13
0559..0569 | - | - | GeneralSettings.Handset Name | Handset Name. Unit: WideChars
056A..056B | - | - | GeneralSettings.unused | Reserved for future use.
056C | - | - | GeneralSettings.Handover CriteriaMode | Handover criteria / Environment muting 0x00=NORMAL 0x01=NOISY 0x02=ENHANCED Range: 0..2
056D | - | - | GeneralSettings.Answer Mode | Answer Mode. 0x00=Normal 0x01=Any Key 0x02=Automatic Range: 0..2
056E | - | - | GeneralSettings.Automatic KeylockTimeout | Automatic Keylock Timeout. 0x00=Off 0x01=Timeout 1 (15s) 0x02=Timeout 2 (30s) 0x03=Timeout 3 (45s) 0x04=Timeout 4 (1m) 0x05=Timeout 5 (2m) 0x06=Timeout 6 (3m) 0x07=Timeout 7 (4m) 0x08=Timeout 8 (5m) Range: 0..8
056F..0571 |  |  | GeneralSettings.LedSetting | LED Setting. See the description of the individual elements below. 0x00=Off 0x01=Missed Call 0x02=Text Message 0x03=Voice Mail 0x04=Text Message or Voice Mail 0x05=Low Battery 0x06=PBX 0x07=Out of Range 0x08=Charging 0x09=Silent Charging 0x0A=Bluetooth Range: 0..7
056F | - | - | GeneralSettings.LedSetting. RedLED | Red LED. Note: See GeneralSettings.LedSetting for description of range and values
0570 | - | - | GeneralSettings.LedSetting. GreenLED | Green LED. Note: See GeneralSettings.LedSetting for description of range and values
0571 | - | - | GeneralSettings.LedSetting. OrangeLED | Orange LED. Note: See GeneralSettings.LedSetting for description of range and values
0572 | - | - | GeneralSettings.Silent ChargingMode | Silent Charging Mode. 0x00=Off 0x01=Silence Range: 0..1
0573 | - | - | GeneralSettings.TimeFormat | Time Format. 0x00=24 Hours 0x01=AM/PM Range: 0..1
0574 | - | - | GeneralSettings.DateFormat | Date Format. 0x00=EU (e.g. 24-02-2012) 0x01=US (e.g. 02/24/2012) 0x02=SP1 (e.g. 24-Feb-2012) 0x03=SP2 (e.g. 24/02/2012) 0x04=SP3 (e.g. 24.02.2012) 0x05=SP4 (e.g. 2012-02-24) Range: 0..5
0575..0577 | - | - | IdleSKShortcutTable | Idle screen softkey shortcuts. Note: See NaviKeyShortcut description of range and values
Address | Value | Type | Name | Description (Various Settings)
0578..057B |  |  | VariousSettings | Various Settings Flags. See description of the individual flags below.
0578 | - | - | VariousSettings.Flags. DemoMode | Demo Mode, where the power safe and deregistration are disabled. 0=disabled 1=enabled
0578 | - | - | VariousSettings.Flags. EncryptionCheck | Protocol-level DECT encryption enabled. 0=disabled 1=enabled
0578 | - | - | VariousSettings.Flags. DefaultCheck | The DefaultCheck flag is set on default and is then used to check if the handset shall be defaulted during reboot. 0=No request for defaulting 1=Request for defaulting
0578 | - | - | VariousSettings.Flags. EconomyMode | Economy Mode, where the handset enters RF low power during periods with high RRSI. 0=disabled 1=enabled
0578 | - | - | VariousSettings.Flags. SerialRamEnabled | Flag to open up for special display mode used when copying display content to PC. 0=disabled 1=enabled
0578 | - | - | VariousSettings.Flags. PhoneLock | Phone Lock, where the used is requested to enter PIN code. 0=disabled 1=enabled
0578 | - | - | VariousSettings.Flags. AccessibilityKeyRepeat | 2 second key repeat 0=disabled 1=enabled
0578 | - | - | VariousSettings.Flags. LockSideFunctionKey |
0579 | - | - | VariousSettings.Flags. SoftkeyImagesEnabled | Softkey mode (Image/text) - ALE feature 0=Off (Images used) 1=On (Text used)
0579 | - | - | VariousSettings.Flags. VibratorShortcut | VibratorShortcut mode - ALE feature 0=Off 1=On
0579 | - | - | VariousSettings.Flags. KeyLock | KeyLock mode - ALE feature 0=Off 1=On
0579 | - | - | VariousSettings.Flags. ForceCalendarRing | ForceCalendarRing mode - ALE feature 0=Off 1=On
0579 | - | - | VariousSettings.Flags. HeadsetMode | HeadsetMode mode - ALE feature 0=Off 1=On
0579 | - | - | VariousSettings.Flags. EasyReply | EasyReply mode - NEC feature 0=Off 1=On
0579 | - | - | VariousSettings.Flags. Clr4MsgHold | CLR key for message hold mode - NEC feature 0=Off 1=On
0579 | - | - | VariousSettings.Flags. CradleDimMode | Set to enable Charger backlight - NEC feature 0=Off 1=On
057A..057B |  |  | VariousSettings.Flags2 |
057A | - | - | VariousSettings.Flags2. SilentModeOverrule | When enabled, the Silent mode overrules message commands (e.g. <<S02,2>>) except NEN messages 0=Off 1=On
057A | - | - | VariousSettings.Flags2. PersonalSafety | Used by NEC DHC tool to identify if Personal Safety is enabled 0=Off 1=On
057A | - | - | VariousSettings.Flags2. NoAnswFromSysPopup |
057A | - | - | VariousSettings.Flags2. Reserved | Reserved
057B | - | - | VariousSettings.Flags2. Reserved2 | Reserved
057C | 01 | fs | CentralDirAvailable | Central Directory available. 0x00 = Disabled. 0x00 = Enabled
057D..0581 |  |  | AgapClockTimerSettings |
057D | 20 | fs | AgapClockTimerSettings. ClockFormat |
057E | 03 | fs | AgapClockTimerSettings. ClockLine |
057F | 00 | fs | AgapClockTimerSettings. ClockColumn |
0580 | 03 | fs | AgapClockTimerSettings. TimerLine |
0581 | 00 | fs | AgapClockTimerSettings. TimerColumn |
0582 | F0 | fs4 | DtmfVolume |
0583..0584 |  |  | VariousSettingsEe |
0583 | - | - | VariousSettingsEe.SdCard Seen |
0583 | - | - | VariousSettingsEe.SdCard Monitoring |
0583 | - | - | VariousSettingsEe.Ignore ChargePowerSave |
0583 | - | - | VariousSettingsEe.Enter ConfigurationMode |
0583 | - | - | VariousSettingsEe.Deprecated_ SoftkeyImagesEnabled |
0583 | - | - | VariousSettingsEe.Deprecated_ KeyLock |
0583 | - | - | VariousSettingsEe.Deprecated_ CradleDimMode |
0583 | - | - | VariousSettingsEe.Deprecated_ ForceCalendarRing |
0584 | - | - | VariousSettingsEe.unused2 |
0585..0588 | - | - | Reserved_VariousSettings | Reserved
0589 | - | - | DockSettings |
0589 | - | - | DockSettings.pwr_on_dock |
0589 | - | - | DockSettings.bck_light_on_remove |
0589 | - | - | DockSettings.answer_call_on_remove |
0589 | - | - | DockSettings.displayBacklight |
0589 | - | - | DockSettings.reserved |
Address | Value | Type | Name | Description (Navigation Key Shortcuts)
058A..058D |  |  | NaviKeyShortcut | Navigation Key Shortcuts. See the description of the individual elements below. 0x00=None 0x01=Messaging 0x02=Send Message 0x03=Inbox 0x04=Sent Messages 0x05=Accessories 0x06=Calculator 0x07=Stopwatch 0x08=Alarms 0x09=Settings 0x0A=Select Profile 0x0B=Time and Date 0x0C=Shortcuts 0x0D=Ringtone 0x0E=Ring Volume 0x0F=Alert Tone 0x10=Alert Volume 0x11=Wallpaper 0x12=Themes 0x13=Answer Mode 0x14=Contacts 0x15=New Contact 0x16=Central Directory (LAS) 0x17=Calls 0x18=Calendar 0x19=Status 0x1A=Voice Mail 0x1B=Vibrator 0x1C=Connectivity 0x1D=Bluetooth 0x1E=Network Select 0x1F=VIP Settings 0x20=Display Settings 0x21=Startup Screen 0x22=Power Safe Timeout 0x23=Reserved, do not use. 0x24=Reserved, do not use. 0x25=Settings Tab Menu 0x26=Missed Calls 0x27=Call Options Range: 0..39
058A | - | - | NaviKeyShortcut.NaviKey Left | Navigation Key Left. Note: See above for description of range and values
058B | - | - | NaviKeyShortcut.NaviKey Up | Navigation Key Up. Note: See above for description of range and values
058C | - | - | NaviKeyShortcut.NaviKey Right | Navigation Key Right. Note: See above for description of range and values
058D | - | - | NaviKeyShortcut.NaviKey Down | Navigation Key Down. Note: See above for description of range and values
Address | Value | Type | Name | Description (Display Settings)
058E..0592 |  |  | DisplaySettings | Display Settings. See the description of the individual elements below.
058E | - | - | DisplaySettings.Display Theme | Display Theme. 0x00=Alcatel Lucent 0x01=Orange 0x02=Choose at startup Range: 0..1
058F | - | - | DisplaySettings.WallPaper Mode | WallPaper Mode. Controlled by DisplayTheme. Range: -
0590 | - | - | DisplaySettings.Startup ScreenMode | Startup Screen Mode. Controlled by DisplayTheme. Range: -
0591 | - | - | DisplaySettings.Power Save.BacklightDimTimeout | Power Save. Backlight Dim Timeout. Unit: Seconds Range: 0..59
0592 | - | - | DisplaySettings.Power Save.BacklightOffTimeout | Power Save. Backlight Off Timeout. Unit: Seconds Range: 0..59
0593 | FF | fs4 | Deprecated_ProfileId |
0594 | - | - | Profile.RingerLevel |
0595 | - | - | Profile.ExtRingerMelody |
0596 | - | - | Profile.IntRingerMelody |
0597 | - | - | Profile.UnknownNumber RingerMelody |
0598 | - | - | Profile.NormalMessage RingerMelody |
0599 | - | - | Profile.UrgentMessage RingerMelody |
059A | - | - | Profile.EmergencyMessage RingerMelody |
059B | - | - | Profile.AlertLevel |
059C | - | - | Profile.AlertMelody |
059D..059E |  |  | Profile.ProfileFlags |
059D | - | - | Profile.ProfileFlags. RingerIncreasingMode |
059D | - | - | Profile.ProfileFlags. VibratorMode |
059D | - | - | Profile.ProfileFlags. KeySoundMode |
059D | - | - | Profile.ProfileFlags. ConfirmationToneMode |
059D | - | - | Profile.ProfileFlags. CoverageWarningMode |
059E | - | - | Profile.ProfileFlags. ChargerWarningMode |
059E | - | - | Profile.ProfileFlags. AlertIncreasingMode |
059E | - | - | Profile.ProfileFlags. LowBatWarningMode |
059E | - | - | Profile.ProfileFlags. ForcedRinging |
059E | - | - | Profile.ProfileFlags. PreviousVibratorMode |
059E | - | - | Profile.ProfileFlags. CoverageWarningFlash |
059F..05A9 | FF..FF | fs1 | Deprecated_Profile |
063B..0660 |  |  | LogCounters |
063B..063C | 00 00 | fs1 | LogCounters.Resets |
063D..063E | 00 00 | fs1 | LogCounters.NewBattery |
063F..0644 | 00 00 00 00 00 00 | fs1 | LogCounters.Reserved_ Power | Reserved
0645..0646 | 00 00 | fs1 | LogCounters.NoAnswFrom SysMAC |
0647..0648 | 00 00 | fs1 | LogCounters.NoAnswFrom SysAPP |
0649..0654 | 00..00 | fs1 | LogCounters.Reserved_ NWK | Reserved
0655..0658 | 00 00 00 00 | fs1 | LogCounters.MaxHeap |
0659..065A | 00 00 | fs1 | LogCounters.MaxMailQueue |
065B..0660 | 00 00 00 00 00 00 | fs1 | LogCounters.Reserved_ OS | Reserved
0661 | 00 | fs4 | BacklightStateSave |
0662..0672 | - | - | Reserved_Display2 | Reserved
Address | Value | Type | Name | Description (Call Settings)
0673..0674 | 00 00 | fs | CallsAnswered | Calls Answered Counter counting the number of answered calls.
0675 | 00 | fs4 | DoNotDisturb | Reject all incoming calls without notifying the user. 0=disabled 1=enabled Note: Not supported
0676 | 00 | f | WideBand | WideBand call enabled in device. 0=disabled 1=enabled
0677 | 00 | fs | EnableTestToneInCall | Test tone routed to audio stream via OK key in call. 0=disabled 1=enabled
0678 | 00 | fs | HACAudioMode |
0679..067C | 00 00 00 00 | fs | CallsDuration | Total Calls Duration. Unit: Seconds
067D | 0A | fs4 | MissedCallTimeout | Missed Call Timeout. Missed calls closed before this timeout will not be logged. Unit: Seconds Range: 0..59
067E..0683 | - | - | Reserved_CallSettings | Reserved
Address | Value | Type | Name | Description (Connectivity Settings)
0684 | - | - | ActiveRegistration |
0685..0690 |  |  | PpEnrolledBases.Element 0 | Enrolled Base 0. See the description of the individual elements below.
0685 | FF | fs | PpEnrolledBases.Element 0.PpHsNo | The handset number at this base.
0686 | FF | fs | PpEnrolledBases.Element 0.IsKnownBase | Is Known Base. 0x00=no 0x01=yes Range: 0..1
0687 | FF | fs | PpEnrolledBases.Element 0.CodecList.Negotiation Indicator | Negotiation Indicator. 0x00=not possible 0x01=possible Range: 0..1
0688 | FF | fs | PpEnrolledBases.Element 0.CodecList.NoOfCodec Entries | Number of Codec entries. Range: 0..2
0689..068C |  |  | PpEnrolledBases.Element 0.CodecList.CodecInfo. Element 0 | Codec Info 0. See the description of the individual elements below.
0689 | FF | fs | PpEnrolledBases.Element 0.CodecList.CodecInfo. Element 0.Codec | Codec setting. 0x00=Codec not specified or not relevant 0x01=user specific, information transfer rate 32 kbit/s 0x02=G.726 ADPCM, information transfer rate 32 kbit/s 0x03=G.722, information transfer rate 64 kbit/s 0x04=G.711 a-law PCM, information transfer rate 64 kbit/s 0x05=G.711 u-law PCM, information transfer rate 64 kbit/s 0x06=G.729.1, information transfer rate 32 kbit/s 0x07=MPEG-4 ER AAC-LD, information transfer rate 32 kbit/s 0x08=MPEG-4 ER AAC-LD, information transfer rate 64 kbit/s 0x09=user specific, information transfer rate 64 kbit/s Range: 0..9
068A | FF | fs | PpEnrolledBases.Element 0.CodecList.CodecInfo. Element 0.MacDlcService | MAC DLC Service setting. 0x00=DLC service LU1, MAC service: In_minimum_delay 0x01=DLC service LU1, MAC service In_normal_delay 0x02=DLC service LU1, MAC service Ip_error_detect 0x03=DLC service LU1, MAC service Ipq_error_detect 0x04=DLC service LU7, MAC service In_normal_delay 0x05=DLC service LU1, MAC service In_normal_delay, framed as TS 102 527-1 [76], clause C.1 Range: 0..5
068B | FF | fs | PpEnrolledBases.Element 0.CodecList.CodecInfo. Element 0.CplaneRouting | C-plane Routing setting. 0x00=CS only 0x01=CS preferred/CF accepted 0x02=CF preferred/CS accepted 0x03=CF only Range: 0..3
068C | FF | fs | PpEnrolledBases.Element 0.CodecList.CodecInfo. Element 0.SlotSize | Slot Size setting. 0x00=Half slot; j = 0 0x01=Long slot; j = 640 0x02=Long slot; j = 672 0x04=Full slot 0x05=Double slot Range: 0..5
068D..0690 |  |  | PpEnrolledBases.Element 0.CodecList.CodecInfo. Element 1 | Codec Info 1 (Same structure as PpEnrolledBases.Element 0.CodecList.CodecInfo.Element 0)
0691..069C |  |  | PpEnrolledBases.Element 1 | Enrolled Base 1 (Same structure as PpEnrolledBases.Element 0)
069D..06A8 |  |  | PpEnrolledBases.Element 2 | Enrolled Base 2 (Same structure as PpEnrolledBases.Element 0)
06A9..06B4 |  |  | PpEnrolledBases.Element 3 | Enrolled Base 3 (Same structure as PpEnrolledBases.Element 0)
06B5..06FC | FF..FF | fs | PpEnrolledBased_Deprecated |
06B5 | FF | fs | PpEnrolledBased_Deprecated. Element 0.PpHsNo |
06B6 | FF | fs | PpEnrolledBased_Deprecated. Element 0.IsKnownBase |
06B7..06C0 |  |  | PpEnrolledBased_Deprecated. Element 0.CodecList |
06B7 | FF | fs | PpEnrolledBased_Deprecated. Element 0.CodecList.Negotiation Indicator |
06B8 | FF | fs | PpEnrolledBased_Deprecated. Element 0.CodecList.No OfCodecEntries |
06B9..06C0 | FF FF FF FF FF FF FF FF | fs | PpEnrolledBased_Deprecated. Element 0.CodecList.Codec Info |
06B9 | FF | fs | PpEnrolledBased_Deprecated. Element 0.CodecList.Codec Info.Element 0.Codec |
06BA | FF | fs | PpEnrolledBased_Deprecated. Element 0.CodecList.Codec Info.Element 0.MacDlc Service |
06BB | FF | fs | PpEnrolledBased_Deprecated. Element 0.CodecList.Codec Info.Element 0.Cplane Routing |
06BC | FF | fs | PpEnrolledBased_Deprecated. Element 0.CodecList.Codec Info.Element 0.SlotSize |
06BD | FF | fs | PpEnrolledBased_Deprecated. Element 0.CodecList.Codec Info.Element 1.Codec |
06BE | FF | fs | PpEnrolledBased_Deprecated. Element 0.CodecList.Codec Info.Element 1.MacDlc Service |
06BF | FF | fs | PpEnrolledBased_Deprecated. Element 0.CodecList.Codec Info.Element 1.Cplane Routing |
06C0 | FF | fs | PpEnrolledBased_Deprecated. Element 0.CodecList.Codec Info.Element 1.SlotSize |
06C1 | FF | fs | PpEnrolledBased_Deprecated. Element 1.PpHsNo |
06C2 | FF | fs | PpEnrolledBased_Deprecated. Element 1.IsKnownBase |
06C3..06CC |  |  | PpEnrolledBased_Deprecated. Element 1.CodecList |
06C3 | FF | fs | PpEnrolledBased_Deprecated. Element 1.CodecList.Negotiation Indicator |
06C4 | FF | fs | PpEnrolledBased_Deprecated. Element 1.CodecList.No OfCodecEntries |
06C5..06CC | FF FF FF FF FF FF FF FF | fs | PpEnrolledBased_Deprecated. Element 1.CodecList.Codec Info |
06C5 | FF | fs | PpEnrolledBased_Deprecated. Element 1.CodecList.Codec Info.Element 0.Codec |
06C6 | FF | fs | PpEnrolledBased_Deprecated. Element 1.CodecList.Codec Info.Element 0.MacDlc Service |
06C7 | FF | fs | PpEnrolledBased_Deprecated. Element 1.CodecList.Codec Info.Element 0.Cplane Routing |
06C8 | FF | fs | PpEnrolledBased_Deprecated. Element 1.CodecList.Codec Info.Element 0.SlotSize |
06C9 | FF | fs | PpEnrolledBased_Deprecated. Element 1.CodecList.Codec Info.Element 1.Codec |
06CA | FF | fs | PpEnrolledBased_Deprecated. Element 1.CodecList.Codec Info.Element 1.MacDlc Service |
06CB | FF | fs | PpEnrolledBased_Deprecated. Element 1.CodecList.Codec Info.Element 1.Cplane Routing |
06CC | FF | fs | PpEnrolledBased_Deprecated. Element 1.CodecList.Codec Info.Element 1.SlotSize |
06CD | FF | fs | PpEnrolledBased_Deprecated. Element 2.PpHsNo |
06CE | FF | fs | PpEnrolledBased_Deprecated. Element 2.IsKnownBase |
06CF..06D8 |  |  | PpEnrolledBased_Deprecated. Element 2.CodecList |
06CF | FF | fs | PpEnrolledBased_Deprecated. Element 2.CodecList.Negotiation Indicator |
06D0 | FF | fs | PpEnrolledBased_Deprecated. Element 2.CodecList.No OfCodecEntries |
06D1..06D8 | FF FF FF FF FF FF FF FF | fs | PpEnrolledBased_Deprecated. Element 2.CodecList.Codec Info |
06D1 | FF | fs | PpEnrolledBased_Deprecated. Element 2.CodecList.Codec Info.Element 0.Codec |
06D2 | FF | fs | PpEnrolledBased_Deprecated. Element 2.CodecList.Codec Info.Element 0.MacDlc Service |
06D3 | FF | fs | PpEnrolledBased_Deprecated. Element 2.CodecList.Codec Info.Element 0.Cplane Routing |
06D4 | FF | fs | PpEnrolledBased_Deprecated. Element 2.CodecList.Codec Info.Element 0.SlotSize |
06D5 | FF | fs | PpEnrolledBased_Deprecated. Element 2.CodecList.Codec Info.Element 1.Codec |
06D6 | FF | fs | PpEnrolledBased_Deprecated. Element 2.CodecList.Codec Info.Element 1.MacDlc Service |
06D7 | FF | fs | PpEnrolledBased_Deprecated. Element 2.CodecList.Codec Info.Element 1.Cplane Routing |
06D8 | FF | fs | PpEnrolledBased_Deprecated. Element 2.CodecList.Codec Info.Element 1.SlotSize |
06D9 | FF | fs | PpEnrolledBased_Deprecated. Element 3.PpHsNo |
06DA | FF | fs | PpEnrolledBased_Deprecated. Element 3.IsKnownBase |
06DB..06E4 |  |  | PpEnrolledBased_Deprecated. Element 3.CodecList |
06DB | FF | fs | PpEnrolledBased_Deprecated. Element 3.CodecList.Negotiation Indicator |
06DC | FF | fs | PpEnrolledBased_Deprecated. Element 3.CodecList.No OfCodecEntries |
06DD..06E4 | FF FF FF FF FF FF FF FF | fs | PpEnrolledBased_Deprecated. Element 3.CodecList.Codec Info |
06DD | FF | fs | PpEnrolledBased_Deprecated. Element 3.CodecList.Codec Info.Element 0.Codec |
06DE | FF | fs | PpEnrolledBased_Deprecated. Element 3.CodecList.Codec Info.Element 0.MacDlc Service |
06DF | FF | fs | PpEnrolledBased_Deprecated. Element 3.CodecList.Codec Info.Element 0.Cplane Routing |
06E0 | FF | fs | PpEnrolledBased_Deprecated. Element 3.CodecList.Codec Info.Element 0.SlotSize |
06E1 | FF | fs | PpEnrolledBased_Deprecated. Element 3.CodecList.Codec Info.Element 1.Codec |
06E2 | FF | fs | PpEnrolledBased_Deprecated. Element 3.CodecList.Codec Info.Element 1.MacDlc Service |
06E3 | FF | fs | PpEnrolledBased_Deprecated. Element 3.CodecList.Codec Info.Element 1.Cplane Routing |
06E4 | FF | fs | PpEnrolledBased_Deprecated. Element 3.CodecList.Codec Info.Element 1.SlotSize |
06E5 | FF | fs | PpEnrolledBased_Deprecated. Element 4.PpHsNo |
06E6 | FF | fs | PpEnrolledBased_Deprecated. Element 4.IsKnownBase |
06E7..06F0 |  |  | PpEnrolledBased_Deprecated. Element 4.CodecList |
06E7 | FF | fs | PpEnrolledBased_Deprecated. Element 4.CodecList.Negotiation Indicator |
06E8 | FF | fs | PpEnrolledBased_Deprecated. Element 4.CodecList.No OfCodecEntries |
06E9..06F0 | FF FF FF FF FF FF FF FF | fs | PpEnrolledBased_Deprecated. Element 4.CodecList.Codec Info |
06E9 | FF | fs | PpEnrolledBased_Deprecated. Element 4.CodecList.Codec Info.Element 0.Codec |
06EA | FF | fs | PpEnrolledBased_Deprecated. Element 4.CodecList.Codec Info.Element 0.MacDlc Service |
06EB | FF | fs | PpEnrolledBased_Deprecated. Element 4.CodecList.Codec Info.Element 0.Cplane Routing |
06EC | FF | fs | PpEnrolledBased_Deprecated. Element 4.CodecList.Codec Info.Element 0.SlotSize |
06ED | FF | fs | PpEnrolledBased_Deprecated. Element 4.CodecList.Codec Info.Element 1.Codec |
06EE | FF | fs | PpEnrolledBased_Deprecated. Element 4.CodecList.Codec Info.Element 1.MacDlc Service |
06EF | FF | fs | PpEnrolledBased_Deprecated. Element 4.CodecList.Codec Info.Element 1.Cplane Routing |
06F0 | FF | fs | PpEnrolledBased_Deprecated. Element 4.CodecList.Codec Info.Element 1.SlotSize |
06F1 | FF | fs | PpEnrolledBased_Deprecated. Element 5.PpHsNo |
06F2 | FF | fs | PpEnrolledBased_Deprecated. Element 5.IsKnownBase |
06F3..06FC |  |  | PpEnrolledBased_Deprecated. Element 5.CodecList |
06F3 | FF | fs | PpEnrolledBased_Deprecated. Element 5.CodecList.Negotiation Indicator |
06F4 | FF | fs | PpEnrolledBased_Deprecated. Element 5.CodecList.No OfCodecEntries |
06F5..06FC | FF FF FF FF FF FF FF FF | fs | PpEnrolledBased_Deprecated. Element 5.CodecList.Codec Info |
06F5 | FF | fs | PpEnrolledBased_Deprecated. Element 5.CodecList.Codec Info.Element 0.Codec |
06F6 | FF | fs | PpEnrolledBased_Deprecated. Element 5.CodecList.Codec Info.Element 0.MacDlc Service |
06F7 | FF | fs | PpEnrolledBased_Deprecated. Element 5.CodecList.Codec Info.Element 0.Cplane Routing |
06F8 | FF | fs | PpEnrolledBased_Deprecated. Element 5.CodecList.Codec Info.Element 0.SlotSize |
06F9 | FF | fs | PpEnrolledBased_Deprecated. Element 5.CodecList.Codec Info.Element 1.Codec |
06FA | FF | fs | PpEnrolledBased_Deprecated. Element 5.CodecList.Codec Info.Element 1.MacDlc Service |
06FB | FF | fs | PpEnrolledBased_Deprecated. Element 5.CodecList.Codec Info.Element 1.Cplane Routing |
06FC | FF | fs | PpEnrolledBased_Deprecated. Element 5.CodecList.Codec Info.Element 1.SlotSize |
06FD..0708 | 00..00 | fs | BroadcastGroups | List of Broadcast Groups. See the description of the individual elements below.
06FD..06FE | 00 00 | fs | BroadcastGroups.Element 0 | Broadcast Group number. Range: 0..999
06FF..0700 | 00 00 | fs | BroadcastGroups.Element 1 | Broadcast Group number. Range: 0..999
0701..0702 | 00 00 | fs | BroadcastGroups.Element 2 | Broadcast Group number. Range: 0..999
0703..0704 | 00 00 | fs | BroadcastGroups.Element 3 | Broadcast Group number. Range: 0..999
0705..0706 | 00 00 | fs | BroadcastGroups.Element 4 | Broadcast Group number. Range: 0..999
0707..0708 | 00 00 | fs | BroadcastGroups.Element 5 | Broadcast Group number. Range: 0..999
0709 | 00 | fs | SelectedNetwork | Selected network. 0x00=Auto select 0x01=Use PpEnrolledBases.Element 0 0x02=Use PpEnrolledBases.Element 1 .... .... 0x0A=Use PpEnrolledBases.Element 9 Range: 0..10
070A..072B |  |  | NetworkData.Element 0 | Network Data 0. See the description of the individual elements below.
070A..071A | FF..FF | fs | NetworkData.Element 0. Name | Network name. Unit: WideChars
071B..072B | FF..FF | fs | NetworkData.Element 0. Number | Network number. Unit: WideChars
072C..074D |  |  | NetworkData.Element 1 | Network Data 1 (Same structure as NetworkData.Element 0)]
074E..076F |  |  | NetworkData.Element 2 | Network Data 2 (Same structure as NetworkData.Element 0)]
0770..0791 |  |  | NetworkData.Element 3 | Network Data 3 (Same structure as NetworkData.Element 0)]
0792..085D | FF..FF | fs | NetworkData_Deprecated |
0792..07A2 | FF..FF | fs | NetworkData_Deprecated. Element 0.Name |
07A3..07B3 | FF..FF | fs | NetworkData_Deprecated. Element 0.Number |
07B4..07C4 | FF..FF | fs | NetworkData_Deprecated. Element 1.Name |
07C5..07D5 | FF..FF | fs | NetworkData_Deprecated. Element 1.Number |
07D6..07E6 | FF..FF | fs | NetworkData_Deprecated. Element 2.Name |
07E7..07F7 | FF..FF | fs | NetworkData_Deprecated. Element 2.Number |
07F8..0808 | FF..FF | fs | NetworkData_Deprecated. Element 3.Name |
0809..0819 | FF..FF | fs | NetworkData_Deprecated. Element 3.Number |
081A..082A | FF..FF | fs | NetworkData_Deprecated. Element 4.Name |
082B..083B | FF..FF | fs | NetworkData_Deprecated. Element 4.Number |
083C..084C | FF..FF | fs | NetworkData_Deprecated. Element 5.Name |
084D..085D | FF..FF | fs | NetworkData_Deprecated. Element 5.Number |
085E..085F | 00 00 | fs | AgapEnrolled | Bitfield identifing AGAP based registrations, e.g. bit1 set = Registration 1 is AGAP. Set by the protocol, do not set manually.
0860..0861 | 00 00 | fs | PowerMode50mwEnabled | Bitfield controlling which registration running in ECO mode, e.g. bit2 set = Registration 2 is running in ECO / 50 mW mode.
0862..0863 | 00 00 | fs | OxoEnrolled | Bitfield identifing Oxo based registrations, e.g. bit1 set = Registration 1 is Oxo. Set by the protocol, do not set manually.
0864..0865 | 00 00 | fs | IPDECTEnrolled | Bitfield identifing IPDECT based registrations, e.g. bit1 set = Registration 1 is IPDECT. Set by the protocol, do not set manually.
087E..087F | 00 00 | fs | LegacySetting |
0880 | - | - | EarlyEncryptionKeyArr. Element 0.DefaultCipker KeyIndexMsb | Internal parameters for the early encryption feature.
0881 | - | - | EarlyEncryptionKeyArr. Element 0.DefaultCipker KeyIndexLsb | Internal parameters for the early encryption feature.
0882..0889 | - | - | EarlyEncryptionKeyArr. Element 0.DefaultCipker KeyArr | Internal parameters for the early encryption feature.
088A | - | - | EarlyEncryptionKeyArr. Element 1.DefaultCipker KeyIndexMsb | Internal parameters for the early encryption feature.
088B | - | - | EarlyEncryptionKeyArr. Element 1.DefaultCipker KeyIndexLsb | Internal parameters for the early encryption feature.
088C..0893 | - | - | EarlyEncryptionKeyArr. Element 1.DefaultCipker KeyArr | Internal parameters for the early encryption feature.
0894 | - | - | EarlyEncryptionKeyArr. Element 2.DefaultCipker KeyIndexMsb | Internal parameters for the early encryption feature.
0895 | - | - | EarlyEncryptionKeyArr. Element 2.DefaultCipker KeyIndexLsb | Internal parameters for the early encryption feature.
0896..089D | - | - | EarlyEncryptionKeyArr. Element 2.DefaultCipker KeyArr | Internal parameters for the early encryption feature.
089E | - | - | EarlyEncryptionKeyArr. Element 3.DefaultCipker KeyIndexMsb | Internal parameters for the early encryption feature.
089F | - | - | EarlyEncryptionKeyArr. Element 3.DefaultCipker KeyIndexLsb | Internal parameters for the early encryption feature.
08A0..08A7 | - | - | EarlyEncryptionKeyArr. Element 3.DefaultCipker KeyArr | Internal parameters for the early encryption feature.
08A8..08E3 | - | - | EarlyEncryptionKeyArr_ Deprecated |
08A8 | - | - | EarlyEncryptionKeyArr_ Deprecated.Element 0. DefaultCipkerKeyIndex Msb |
08A9 | - | - | EarlyEncryptionKeyArr_ Deprecated.Element 0. DefaultCipkerKeyIndex Lsb |
08AA..08B1 | - | - | EarlyEncryptionKeyArr_ Deprecated.Element 0. DefaultCipkerKeyArr |
08B2 | - | - | EarlyEncryptionKeyArr_ Deprecated.Element 1. DefaultCipkerKeyIndex Msb |
08B3 | - | - | EarlyEncryptionKeyArr_ Deprecated.Element 1. DefaultCipkerKeyIndex Lsb |
08B4..08BB | - | - | EarlyEncryptionKeyArr_ Deprecated.Element 1. DefaultCipkerKeyArr |
08BC | - | - | EarlyEncryptionKeyArr_ Deprecated.Element 2. DefaultCipkerKeyIndex Msb |
08BD | - | - | EarlyEncryptionKeyArr_ Deprecated.Element 2. DefaultCipkerKeyIndex Lsb |
08BE..08C5 | - | - | EarlyEncryptionKeyArr_ Deprecated.Element 2. DefaultCipkerKeyArr |
08C6 | - | - | EarlyEncryptionKeyArr_ Deprecated.Element 3. DefaultCipkerKeyIndex Msb |
08C7 | - | - | EarlyEncryptionKeyArr_ Deprecated.Element 3. DefaultCipkerKeyIndex Lsb |
08C8..08CF | - | - | EarlyEncryptionKeyArr_ Deprecated.Element 3. DefaultCipkerKeyArr |
08D0 | - | - | EarlyEncryptionKeyArr_ Deprecated.Element 4. DefaultCipkerKeyIndex Msb |
08D1 | - | - | EarlyEncryptionKeyArr_ Deprecated.Element 4. DefaultCipkerKeyIndex Lsb |
08D2..08D9 | - | - | EarlyEncryptionKeyArr_ Deprecated.Element 4. DefaultCipkerKeyArr |
08DA | - | - | EarlyEncryptionKeyArr_ Deprecated.Element 5. DefaultCipkerKeyIndex Msb |
08DB | - | - | EarlyEncryptionKeyArr_ Deprecated.Element 5. DefaultCipkerKeyIndex Lsb |
08DC..08E3 | - | - | EarlyEncryptionKeyArr_ Deprecated.Element 5. DefaultCipkerKeyArr |
08E4..094F | - | - | Reserved_BluetoothSettings | Reserved
0950..098F | 00..00 | fs1 | RosLogEntries |
0990..0A8F | 00..00 | fs1 | LogStack |
0A90..0AC1 |  |  | NoAnswerFromSysLogs |
0A90..0AC1 | 00..00 | fs1 | NoAnswerFromSysLogs.Log |
0A90 | 00 | fs1 | NoAnswerFromSysLogs.Log. Element 0.Reason |
0A91 | 00 | fs1 | NoAnswerFromSysLogs.Log. Element 0.OriginTask |
0A92..0A95 | 00 00 00 00 | fs1 | NoAnswerFromSysLogs.Log. Element 0.TimeStamp |
0A96..0A99 | 00 00 00 00 | fs1 | NoAnswerFromSysLogs.Log. Element 0.Reserved | Reserved
0A9A | 00 | fs1 | NoAnswerFromSysLogs.Log. Element 1.Reason |
0A9B | 00 | fs1 | NoAnswerFromSysLogs.Log. Element 1.OriginTask |
0A9C..0A9F | 00 00 00 00 | fs1 | NoAnswerFromSysLogs.Log. Element 1.TimeStamp |
0AA0..0AA3 | 00 00 00 00 | fs1 | NoAnswerFromSysLogs.Log. Element 1.Reserved | Reserved
0AA4 | 00 | fs1 | NoAnswerFromSysLogs.Log. Element 2.Reason |
0AA5 | 00 | fs1 | NoAnswerFromSysLogs.Log. Element 2.OriginTask |
0AA6..0AA9 | 00 00 00 00 | fs1 | NoAnswerFromSysLogs.Log. Element 2.TimeStamp |
0AAA..0AAD | 00 00 00 00 | fs1 | NoAnswerFromSysLogs.Log. Element 2.Reserved | Reserved
0AAE | 00 | fs1 | NoAnswerFromSysLogs.Log. Element 3.Reason |
0AAF | 00 | fs1 | NoAnswerFromSysLogs.Log. Element 3.OriginTask |
0AB0..0AB3 | 00 00 00 00 | fs1 | NoAnswerFromSysLogs.Log. Element 3.TimeStamp |
0AB4..0AB7 | 00 00 00 00 | fs1 | NoAnswerFromSysLogs.Log. Element 3.Reserved | Reserved
0AB8 | 00 | fs1 | NoAnswerFromSysLogs.Log. Element 4.Reason |
0AB9 | 00 | fs1 | NoAnswerFromSysLogs.Log. Element 4.OriginTask |
0ABA..0ABD | 00 00 00 00 | fs1 | NoAnswerFromSysLogs.Log. Element 4.TimeStamp |
0ABE..0AC1 | 00 00 00 00 | fs1 | NoAnswerFromSysLogs.Log. Element 4.Reserved | Reserved
0AC2..0ACF | - | - | Reserved_Debug | Reserved
0AD0 | - | - | GeneralSettings2 | General Settings 2. See the description of the individual elements below.
0AD0 | - | - | GeneralSettings2.Screen SaverDelay | Screen Saver Delay. 0x00=5s 0x01=10s 0x02=20s 0x03=30s 0x04=45s 0x05=60s Range: 0..5
0AD1..0AE5 | - | - | ProxyPassword | Network Proxy Password. Unit: Chars
0AE6..0AEF | - | - | Reserved_GeneralSettings2 | Reserved
Address | Value | Type | Name | Description (Alarm Settings)
0AF0..0AF8 |  |  | AlarmSettings | Alarm Settings. See the description of the individual elements below.
0AF0 | - | - | AlarmSettings.AlarmTime. Hour | Hours setting for normal alarm. Unit: Hours Range: 0..23
0AF1 | - | - | AlarmSettings.AlarmTime. Minute | Minutes setting for normal alarm. Unit: Minutes Range: 0..59
0AF2 | - | - | AlarmSettings.Recurrent AlarmTime.Hour | Hours setting for recurrent alarm. Unit: Hours Range: 0..23
0AF3 | - | - | AlarmSettings.Recurrent AlarmTime.Minute | Minutes setting for recurrent alarm. Unit: Minutes Range: 0..59
0AF4 | - | - | AlarmSettings.AlarmStatus | Alarm Status Flags. See description of the individual flags below.
0AF4 | - | - | AlarmSettings.AlarmStatus. AlarmEnabled | Alarm Status Flags. Normal alarm enabled. 0=disabled 1=enabled
0AF4 | - | - | AlarmSettings.AlarmStatus. RecurrentAlarmEnabled | Alarm Status Flags. Recurrent alarm enabled. 0=disabled 1=enabled
0AF4 | - | - | AlarmSettings.AlarmStatus. AlarmExpired | Alarm Status Flags. Normal alarm has expired. 0=false 1=true Note: Not supported
0AF4 | - | - | AlarmSettings.AlarmStatus. RecurrentAlarmExpired | Alarm Status Flags. Recurrent alarm has expired. 0=false 1=true Note: Not supported
0AF5 | - | - | AlarmSettings.Checked Days | Checked Days flags. See description of the individual flags below.
0AF5 | - | - | AlarmSettings.Checked Days.Monday | Checked Days flags. Recurrent alarm enabled on mondays. 0=false 1=true
0AF5 | - | - | AlarmSettings.Checked Days.Tuesday | Checked Days flags. Recurrent alarm enabled on tuesdays. 0=false 1=true
0AF5 | - | - | AlarmSettings.Checked Days.Wednesday | Checked Days flags. Recurrent alarm enabled on wednesdays. 0=false 1=true
0AF5 | - | - | AlarmSettings.Checked Days.Thursday | Checked Days flags. Recurrent alarm enabled on thursdays. 0=false 1=true
0AF5 | - | - | AlarmSettings.Checked Days.Friday | Checked Days flags. Recurrent alarm enabled on fridays. 0=false 1=true
0AF5 | - | - | AlarmSettings.Checked Days.Saturday | Checked Days flags. Recurrent alarm enabled on saturdays. 0=false 1=true
0AF5 | - | - | AlarmSettings.Checked Days.Sunday | Checked Days flags. Recurrent alarm enabled on sundays. 0=false 1=true
0AF6 | - | - | AlarmSettings.SnoozeInterval | Alarm Snooze Interval. Unit: Minutes Range: 1..10
0AF7 | - | - | AlarmSettings.AlarmSnooze Cnt | Alarm Snooze Counter counting the number of snoozes for the latest normal alarm.
0AF8 | - | - | AlarmSettings.Recurrent AlarmSnoozeCnt | Recurrent Alarm Snooze Counter counting the number of snoozes for the latest recurrent alarm.
Address | Value | Type | Name | Description (Calendar Settings)
0AFE..0B0D |  |  | CalendarSettings | Calendar Settings. See description of the individual elements below.
0AFE | - | - | CalendarSettings.View Mode | Calendar Settings. Calendar View Mode 0x00=Month View 0x01=Week View Range: 0..1
Address | Value | Type | Name | Description (Message Settings)
0B0E | 05 | fs | LrmsFlags | LRMS Flags. See description of the individual flags below.
0B0E | xxxxxxx1 | fs | LrmsFlags.OverwriteOld | LRMS Flags. Overwrite old messages when there is no free memory left for storing a new message. 0=disabled 1=enabled
0B0E | xxxxxx0x | fs | LrmsFlags.SendMessages | LRMS Flags. Store sent messages. 0=disabled 1=enabled
0B0E | xxxxx1xx | fs | LrmsFlags.Display | LRMS Flags. Display the incoming message in a viewer if enabled, otherwise prompt the user before showing the message. 0=disabled 1=enabled
0B0E | xxxx0xxx | fs | LrmsFlags.AutoAnswerMsg | LRMS Flags. Allow auto answer enabled via incoming message. 0=disabled 1=enabled
0B0E | xxx0xxxx | fs | LrmsFlags.SilentAnswer Msg | LRMS Flags. Allow silent answer enabled via incoming message. 0=disabled 1=enabled
0B0F..0B2E | 00..00 | fs | LrmsVoiceMailNumber | Voice Mail number. Unit: Chars
0B2F..0B30 | 00 00 | fs | MessageCount | Number of successfully sent messages.
Address | Value | Type | Name | Description (List Manager)
0B38..0B49 | FF..FF | fs | GroupAttributeList |
0B7C..0BDF | FF..FF | fs | LmCallLogList |
0C44..0C50 | FF..FF | fs | SpeedDialNumberList |
0C5D..0C6F | FF..FF | fs | StorageManagerFAT |
0C70..31EF | - | - | StorageManagerDataArea |
31F0..3FFF | - | - |  |